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CENTRAL BANK OF INDIA- REGIONAL OFFICE-GWALIOR
 NOTICE OF INVITATION TO TENDER 











DATE:  09.06.2017
To,
Eligible Contractors 

Sub: Interior, Electrical & AIR CONDITIONING Works of REGIONAL OFFICE-GWALIOR. 

Sealed tenders on item rate basis are invited for works at RO GWALIOR in Two Bid format. Tender Document may be purchased from General Administration Department, Central Bank of India, Regional Office at GWALIOR, against payment of Rs 500.00 by way of DD favoring Central Bank of India, Regional office- GWALIOR (non-refundable) or may be download from bank’s website www.centralbank.co.in & submit it with Rs. 500.00 DD favoring Central Bank of India, Regional office- GWALIOR (non-refundable).

Eligibility Criteria:
Contractors who fulfill the following requirements shall be considered as eligible bidder:

1. Average Annual financial turnover during the last 3 years, ending 31st March of the previous financial year, should be at least 30% of the estimated cost. The bidder should be in profit in the past three years.
2. Experience of having successfully completed similar works during last 3 years ending last day of month previous to the one in which applications are invited executer under Central Government Department/State Government Department/Central Public Sector undertaking should be either of the following:-

a. Three (03) similar completed works costing not less than the amount equal to 40% of the estimated cost.
b. Two (02) similar completed works costing not less than the amount equal to 60% of the estimated cost.
c. One (01) similar completed work costing not less than the amount equal to 80% of the estimated cost.

3. Have registered office in Madhya Pradesh state.

4. Must have valid PAN, TIN, Service tax registration number.
5. Must have EPF/ESI registration.
6. SOLVENCY certificate of amount equals to 40% of the estimated cost of the work.

7. Similar works shall mean Renovation/refurbishing works i.e., combination of interior, furniture works, air conditioning, data & electrical works at bank’s administrative office premises /govt. institutes.
8. Completion certification with regards to the works mentioned for experience (point 2) to be issued by Competent Authority will only be considered as credential. If the Completion certificate issued by Competent Authority does not reflect the type of work, then Final bill / Schedule of Quantity of the qualifying works also to be attached along with the Completion certificates. 

	 S.No.
	PARTICULARS
	DETAILS

	1
	Estimated Cost of Work:
	85 Lacs

	2
	Earnest Money: by crossed D.D. 
	Rs. 85,000.00

	3
	In Favor Of 
	Central Bank Of India, GWALIOR

	4
	Time of Completion:
	60 Days.

	5
	Time & Date of submission of Tender
	On or before 3.00 pm on dated 26.06.2017

	6
	Time & date of opening of Technical Bid
	3.30 pm on dated 26.06.2017

	7
	Financial Bid submitted in separate envelope. Tender having financial bid with technical bid in same envelope will be rejected.


Sr. Regional Manager

Central Bank of India

Regional Office,

GWALIOR.
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FORM OF TENDER

To,

The Sr. Regional Manager,

Central Bank of India,
Regional Office, 

GWALIOR.
NAME OF WORK: Interior, Electrical, Civil, Data & A.C. Works for Regional Office GWALIOR.
Sir,

1.   
Having  visited the site and examined the drawings, conditions  of contract,  special  conditions of contract,  General  specifications  and detailed  specifications, schedules and bill of quantities for  the  construction  of the above named works, we offer to construct, complete  and maintain  the whole of the said works in conformity with the  said  drawings,  conditions  of  contract, specifications, schedules  and  bill  of quantities for the sum State in bill of quantities of this Tender  Document or such other sum as may be ascertained in accordance with the  said conditions of contract.

2.   
We undertake to complete and deliver the whole of the works comprised in the contract within the time State in the appendix hereto.

3.   
We have independently considered the amount of liquidated  damages shown  in  the Appendix hereto  and agree that it represents a  fair  estimate  of  the loss likely to be suffered, by you in the  event  of  the works not being completed in time.

4.   
We  agree to abide by this tender for the period of 90  days  from opening  of envelope  or extension there of as required by the  employer from  the date fixed for receiving the same and it shall  remain  binding upon us and may be accepted at any time before the expiry of that period.

5.   
We  confirm that the period and rates as referred in the  agreement or general conditions of contract are given or summarized in the appendix hereto, to which we give our consent and agree to abide by the same.

6.   
If this tender is accepted, we undertake to enter into and execute at our cost, when called upon by the employer to do so, a contract agreement in the prescribed form. Unless and until a formal agreement is prepared and executed this tender together with your written acceptance there of, shall constitute a binding contract between us.

7.   
We understand that if our tender is accepted, we are to be jointly and severally responsible for the due performance of the contract.

8.   
We  understand that you are not bound to accept the Lowest or  any tender  you may receive and may reject all or any tender, accept  or  entrust  the entire work to the contractor or divide the work to more  than one  contractor  without assigning any reason or giving  any  explanation whatsoever.

Seal & Signature of

Contractor(s)/ Firm
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APPENDIX TO FORM OF TENDER
	Defects Liability period
	12 Months from the date of virtual completion.

	Date of commencement
	07 days from the date of acceptance letter is issued to contractor or day on which the contractor is instructed to take possession of the site whichever is later.

	Time of completion
	60 Days from the date of commencement.

	Period of Final Measurement
	One month from the date of virtual completion

	Liquidated damages
	1%   of   the tendered   amount   shown   in   the tender per week subject to the ceiling of 10% of the accepted contracted sum.

	Minimum value of work for

interim certificate/bill
	Rupees 20 lakhs 

	Initial Security Deposit
	2% of accepted value of tender including the earnest money deposit is to be paid by contractor on acceptance of work order.

	Retention percentage
	8.00% of the cost of the work of the accepted tender amount from each interim bill.

	Refund of total security comprising of EMD, Intial security deposit, Retention Money
	50% of money will be released on issue of virtual completion certificate by engineer/regional office. Remaining 50 %of Total Security deposit will be released 14 days after the end of the defect liability period & upon receipt of “no defect certificate” from the Regional Office/engineer.

	Period of honoring Certificate
	15 days   from date of receipt of certificate from the Bank’s Engineer.


ARTICLES OF AGREEMENT
This agreement made this……………………………..day of ……………………………..two thousand twelve between Central Bank Of India, a body corporate constituted under the Banking Companies (Acquisition & Transfer of Undertaking) Act 1970, having its Head Office at MUMBAI (herein after called “The Employer”) of the ONE PART and M/s ……………………………………………………. herein after called “The Contractor” which includes it’s heir/successors (herein after called “the Guarantor”)of the OTHER PART. 
WHEREAS the Employer is desirous of certain works should be executed viz. Interior Works for Central Bank Of India- Regional Office & has by letter of acceptance dated _________________ accepted a tender by the contractor for the execution, completion, and maintenance of such works, now THIS AGREEMENT WITNESSES as follows :

4.1 In this agreement words & expressions shall have the same meaning as are respectively assigned to them in the said conditions of contract hereinafter referred to:

4.2 The following documents shall be deemed to form & to read construed as part of this agreement, viz.

 i) Original tender document. ii) Relevant correspondence all letters/correspondence forming part of contract and referred to in acceptance letter. iii) Acceptance letter. iv)  Bill of quantities. v) The drawings. vi) Time and progress chart. vii) Other additional documents as required,

a)
b)
c)
viii) Article of Agreement.

4.3 The aforesaid documents shall be taken as complementary and mutually explanatory of one another, but in the case of ambiguities of discrepancies the latest documents issued by the Bank shall prevail over on earlier documents.
 4.4 In consideration of the payment to be made by the employer to the contractor as hereinafter mentioned, the contractor hereby covenants with the employer to perform execute, complete and maintain the work in conformity in all respects with the provision of the contract. 

4.5 The employer hereby covenants to pay the contractor in consideration of the execution, completion and maintenance of the works such sums as shall become payable hereunder at the time(s) and in the manner prescribed in the said conditions and price schedule of quantities/bill of quantities prescribed in the contract.

IN WITNESS where of the parties here to have caused their respective common seals to be hereunto affixed (or have here un to set their respective hands and seals) the day, month and year first above written.

SIGNED AND SEALED AND DELIVERED BY THE

Said ______________________   



said _________________________

(Name _____________________)   


           (Name________________________)

on behalf of the contractor

 


on behalf of the employer

In the presence of 





In the presence of 

Name: ______________   




Name: _______________________

Address: ___________________   



Address: ____________________

 ___________________________   



____________________________

 * This form is included in the tender documents only for the information of the tenderers. Only the successful tenderer will be, in due course, required to complete the form.

[image: image5.emf]
SECTION I
GENERAL RULES & INSTRUCTIONS FOR THE GUIDANCE OF TENDERERS
1.0 Tenders are hereby invited on behalf of Central Bank of India- Regional Office- GWALIOR for the Interior furnishing, Electrical, Air conditioning works of RO GWALIOR.
Contract documents consisting of the plans, complete specifications, the schedule of quantities of the various classes of work to be done and the set of conditions of contract to be complied with by the person/firm whose tenders may be accepted and which will also be found in the form of tenders, can be seen/purchased at the Central Bank Of India, Regional Office GWALIOR between normal working hours of one day prior to the last day of submission of the tenders & except on Sundays & Bank holidays. The site for the work is available 

2.0 Tenders, which should always be placed in sealed cover, with the name of the project written on the envelope will be received by The Deputy Regional Manager, up to 26.06.17 at 3.00P.M. & will be opened by him in his office on dated 26.06.17 at 3.30 hrs.

3.0 In case of two part tenders, dates of submission opening of the tenders & the part thereof along with the superscription on the packages should be as per specific instruction on the tender notice/ form.

4.0 Tenders are to be on the prescribed form which can be obtained from the office of The Senior Regional Manager, Central Bank of India, Regional Office, GWALIOR on payment of a sum of Rs 500.00, in DD Favoring Central Bank Of India-GWALIOR.
5.i
The time allowed for the carrying out of the work will be 60 days from the date of commencement of the work.

5.0 The Contractors should quote in figures as well as in words the rate, & amount tendered by them. The amount for each item should be worked out & the requisite totals given.

6.0  While a contractor signs a tender in an Indian language the percentage above or below & tendered amount & the total amount tendered should also be written in the same language. In the case of illiterate contractors the rates or the amounts tendered should be attested by a witness.

7.0 Issue of tender form will be stopped one day before the date fixed for the opening of tenders.

8.0 Earnest money, amounting to Rupees Eighty Five Thousand  ( Rs. 85,000.00 Only), in the form of Bank Draft drawn in favor of Central Bank Of India” GWALIOR, must accompany each tender and each tender is to be in a sealed cover super scribed "Tender for Interior Works for RO GWALIOR and addressed to The Senior Regional Manager, Central Bank Of India, Regional Office, GWALIOR, (M.P.) 
The EMD of the contractor, whose tender is accepted, shall be fortified in full in case he does not remit the Initial Security Deposit within the stipulated period or start the work by the stipulated date mentioned in the award letter.

9.0 The acceptance of a tender will rest with the Central Bank of India, The Bank reserves the right to accept or reject any or all the tenders received without the assignment of any reasons. All tenders in whom any of the prescribed conditions are not fulfilled or are incomplete in any respect are liable to be rejected.

The bank reserves the right to accept the tender in full or in parts and that tenderer shall have no claim for revision of rates or other conditions if the tender is accepted in parts.   

10.0 Canvassing in connection with tender is strictly prohibited and the tenders submitted by the contractor who resorts to canvassing will be liable to rejection.

11.0 All item rates shall be quoted on the proper form of the tender alone.

12.0 An item rate tender containing percentage below/above will be summarily rejected. However, where a tenderer voluntarily offers a rebate for payment within a stipulated period, this may be considered.

13.0 On  acceptance of tender, the name of the  accredited  representative(s)  of the contractor who would be responsible for  taking  instructions   from  the  Employer/Architect  shall  be  communicated   to   the Employer.
14.0 Special Care should be taken to write the rates in figures as well as in words & the amounts in figures only, in such a way that interpretation is not possible. The total amount should be written both in figures & in words. In case of figures, the words “Rs” should be written before the figure of rupees & words “P” after the decimal figures, e.g. Rs.2.15p. & in case of words, the word “Rupees” should precede & the word “Paisa” should be written at the end, unless the rate ids in whole rupees & followed by the words “Only”, it should invariably be up to two decimal places. While quoting the rates in schedule of quantities, the word “Only” should be written closely following the amount & it should not be written in the next line. 

15.0 The bank does not bind itself to accept the lowest or any tender and reserves to itself the right of accepting the whole or any part of the tender and the tenderer shall be bound to perform the same at the rate quoted. 

16.0 All taxes including Sales Tax or any other tax on material or finished works like’s work’s contract tax, turnover tax etc. in respect of this contract & the Bank will not entertain any claim whatsoever in this respect.
17.0 The contractor shall give a list of his relatives working with the bank along with their designations and addresses.

18.0 No employee of the Bank is allowed to work under or as a contractor for a period of two years after his retirement from Bank services, without the previous permission of the Bank. The contract is liable to be cancelled if either the contractor or any of his employees is found at any time to be such a person who had not obtained the permission of the Bank as aforesaid before submission of the tender or engagement in the contractor's service.

19.0 The tender for works shall remain open for acceptance for a period of 90 days from the date of opening of the tenders.  If any tenderer withdraws his tender before the said period, then bank shall be at liberty to forfeit Earnest Money paid along with the tender.

20.0 The tender for the work shall not be witnessed by a contractor or contractors who himself/themselves has/have tendered or who may and has/have tendered for the said work. Failure to observe this condition would render tenders of the contractors tendering as well as witnessing the tender liable to summary rejection.

21.0 It will be obligatory on the part of the tenderer to tender and sign the tender documents for all the component parts and that, after the work is awarded, he will have to enter in to an agreement, for each component with the competent authority in the bank.

The tenderer, apart from being a competent contractor must associate himself with the agencies of the appropriate class who are eligible for (i) Electrical (ii) Sanitary & water supply installations and (iii) Horticulture.

Signature of the Competent Authority,

CENTRAL BANK OF INDIA, REGIONAL OFFICE-     Gwalior
SECTION II
GENERAL CONDITIONS OF CONTRACT
Except  where provided for in the description of the individual items  in the Schedule of Quantities & in the specifications & conditions  laid down  hereinafter & in the drawings, the work shall be carried  as  per standard  specifications & under the directions of the  Employer/Architects.

1.   
INTERPRETATION

In  construing  these  conditions, the specifications,  the  schedule  of quantities,  tender  & Agreement, the following words  shall  have  the meaning  herein  assigned  to them except where the  subject  of  context otherwise requires :

i) Employer: The term employer shall denote Central Bank Of India with their head office, at MUMBAI, & any of its employees or representative authorized to act on their behalf.

ii) Architects/Consultants: The term Architects/Consultants shall mean Bank’s Engineer or in the event of his/their ceasing to be the Architects for the purpose of this contract such other person/s as the Employer shall nominate for the purpose. The architect with the approval of the Bank may engage a local Architect/ Consulting Engineer for supervision & co- ordination of the work at the site. He will be considered a representative of the Architect. The Bank may also engage a Project Management Consultant for the supervision of the work. He will be designated by the term PMC & work a s Employer’s agent at the site.
iii) Contractor: The term Contractor shall mean …………………………………………….(name & address of the  contractor) & his/their heirs, legal representatives assigns & successors.

iv) Site : The site shall mean the site where the works are to be executed as shown within boundary on the Site Plan including any building & erections there on allotted by the Employer for the Contractor’s use.

v) Site Engineer: The Site Engineer shall be appointed by the Bank. The Bank may also determine the number of Site Engineers & the supporting staff at site office to assist them & also whether the Site Engineer shall be temporary or permanent. As far as possible, the Site Engineer should assume charge of his post before the Contractor reports on site of work. Where more than one Site Engineer is appointed, one of them shall be designated as senior Site Engineer by the Premises Department & the other Site Engineers shall be reporting to the Senior Site Engineer. Wherever PMC is engaged, Site Engineer, if any, will work in close co-ordination with PMC.

vi) Drawings : The work is to be carried out in accordance  with drawings,  specifications,  the schedule of quantities  &  any  further drawings  which  may be supplied or any other instruction, which  may  be given by the employer during the execution of the work.
All the drawings relating to work given to the contractor together with a copy  of  schedule  of  quantities  are  to  be  kept  at  site  &  the Employer/Architects/PMC  shall be given access to such drawings or  schedule  of quantities whenever necessary.

In case any detailed Drawings are necessary, contractor shall prepare such detailed drawings &/or dimensional sketches therefore & have it confirmed by the Employer/Architects/PMC as case may be prior to taking up such work.

The  contractor  shall ask in writing for all clarifications  on  matters occurring  anywhere in  drawings, specifications & schedule of  quantities  or to additional instructions at least 10 days ahead from the  time when it is required for implementations so that the Employer may be  able to give decision thereon.

vii)
"The works" shall mean the work or works to be executed or done under this contract.

viii)
"Act of Insolvency" shall mean any act as such as defined by the Presidency Towns Insolvency Act or in Provincial Insolvency Act or any Amending Statutes.

ix)
"The Schedule of Quantities" shall mean the schedule of quantities as specified & forming part of this contract.

x)
"Priced Schedule of Quantities" shall mean the schedule of quantities duly priced with the accepted quoted rates of the contractor.

2.   SCOPE

The work consists of Interior Works Central Bank Of India- Regional Office, Gwalior, in accordance with the “Drawings" & "Schedule of Quantities". The Interior works, related civil and electrical works etc. complete are within the scope of this tender. It includes furnishing all materials, labor, tools and equipment and management necessary for, and incidental to, the construction & completion of the work. All work, during its progress and upon completion shall confirm to the lines, elevations and grades as shown on the drawings furnished by the Employer/Architects. Should any detail essential  for efficient completion of the work be omitted from the drawings &  specifications it shall be the responsibility of the contractor to inform  the Employer/Architects  & to furnish & install such detail with Employer's / Architect’s  concurrence,  so  that upon completion of the proposed work the  same  will  be acceptable and ready for use.

Employer or his agent (PMC)  may in their absolute discretion issue further drawings  and/or written  instructions, details, directions and explanations,  which  are, hereafter  collectively, referred to as "The Employer's / Architect’s instructions"  in regard to :

a)
The variation or modification of the design quality or quantity of works or the addition or omission or substitution of any work.

b)
Any discrepancy in the drawing or between the schedule of quantities and/or drawings and/or specifications.

c)
The  removal  from  the site of any  defective  materials  brought thereon  by  the contractor and the substitution of  any  other  material thereof.

d)
The demolition/removal and/or re-execution of any work executed by the contractors.

e)
The dismissal from the work of any persons employed thereupon.   

f)
The opening up for inspection of any work covered up.

g)
The rectification and making good of any defects under clauses hereinafter mentioned and those arising during the maintenance period (retention period).

The  contractor  shall forthwith comply with and duly  execute  any  work comprised  in such Employer's or his Agent/ Architect’s instructions, provided always  that  verbal instructions,  directions and explanations given to the  contractor's  or his  representative upon the works by the Employer's or his Agent/ Architect’s shall, if  involving  a variation, be confirmed in writing to the contractor/s within seven  days. No works, for which rates are not specifically mentioned in the priced schedule of quantities, shall be taken up without written permission of the Employer's or his Agent/ Architect’s.  Rates of items not mentioned in the priced schedule of quantities shall be fixed by the employer in consultation with the Architects as provided in clause "variations".

Regarding all factory made products for which ISI marked products are available, only products bearing ISI marking shall be used in the work.

3.   TENDERER SHALL VISIT THE SITE

Intending  Tenderer  shall  visit the site &  make  himself  thoroughly acquainted with the local site conditions, nature and requirements of the works,  facilities of transport conditions, effective labour and  materials,  accesses  and  storage for materials.  The Tenderer shall provide in their tender for cost of carriage, freight and other charges as also for any special difficulties and including police restriction for transport etc. for proper execution of work as indicated in drawings. The successful Tenderer will not be entitled to any claim of compensation for difficulties faced or losses incurred on account of  any site  conditions  which existed before the commencement of  the  work  or which  in the opinion of the Employer might be deemed to have  reasonably been inferred to be so existing before commencement of work.

4. TENDERS
 The entire set of tender paper issued to the tenderer should be submitted fully priced and also signed on the last page together with initials on every page. Initials/Signature will indicate the acceptance of the tender papers by the tenderers.

(Also see para 16 of General Rules & Instructions for the Guidance of Tenderers).

The schedule of quantities shall be filled in as follows:

i)
The “Rate” column to be legibly filled in ink in both English figures and English words.

ii)
Amount column to be filled in for each item and the amount for each subhead as detailed in the "Schedule of Quantities".

iii)
All corrections are to be initialed.

iv)
The "Rate Column" for alternative items shall be filled up.

 v)
The “Amount" column for alternate items of which the quantities are not mentioned shall not be filled up.

vi)
In case of any errors/omissions in the quoted rates, the rates given in the tender marked "Original" shall be taken as correct rates.

No  modifications, overwriting or corrections can be made in  the  tender papers  by the tenderer, but he may at his option offer his  comments  or modifications  in  a  separate sheet of paper attached  to  the  original tender papers.

The employer reserves the right to reject the lowest or any tender and also to discharge any or all of the tenders for each section or to split up and distribute any item of work to any specialist firm or firms, without assigning any reason. The Bank reserves the right to accept the tender in full or in part and the tenderer shall have no claim for revision of rate or other conditions if his tender is accepted in parts.

The tenderers should note that the tender is strictly on the item rate basis and their attention is drawn to the fact that the rates for each and every item should be correct workable and self-supporting. If called upon by the Employer / Architects detailed analysis of any or all the rates shall be submitted by the contractor. The Employer / Architects shall not be bound to recognize the contractor's analysis.

The works will be paid for as "measured work" on the basis of actual work done and not as "lump sum" contract.

All  items  of  work described in the schedule of quantities  are  to  be deemed  and paid as complete works in all respects and details  including preparatory and finishing works involved directly related to and  reasonably detectable from the drawings, specifications and schedule of quantities and no further extra charges will be allowed in this connection.  In the  case  of lump sum charges in the tender in respect of  any  item  of works, the payment of such items of work will be made for the actual work done  on the basis of lump sum charges as will be assessed to be  payable by the employer.

The  employer has power to add to, omit from any works as shown in  drawings or described in specifications or included in schedule of quantities and  intimate the same in writing but no addition, omission or  variation shall be made by the contractor without authorization from the  Employer. No variation shall vitiate the contract.

The tenderer shall note that his tender shall remain open for consideration for a period of 90 days from the date of opening of the tender.
5.   AGREEMENT
The successful contractor may be required to sign agreement as may be drawn up to suit local conditions and shall pay for all stamps and legal expenses, incidental thereto.

6.   GOVERNMENT AND LOCAL RULES
The contractor shall conform to the provisions of all local By-laws and acts relating to the work and to the regulations etc. of the Government and local authorities and of any company with whose system the structure is proposed to be connected. The contractor shall give all notices required by said act, rules, regulations and Byelaws etc. and pay all fees payable to such authorities for execution of the work involved. The cost, if any, shall be deemed to have been included in his quoted rates, taking into account all liabilities for licenses, fees for footpath encroachment and restorations etc. He shall indemnify the employer against such liabilities   and shall defend all actions arising from such claims or liabilities.

7.   TAXES AND DUTIES
The tenderers must include in their tender prices quoted for all duties, royalties, cesses and sales tax, or any other taxes or local charges, if applicable. However, work contract tax shall be deducted at source at the specific rate in Union legislative, if applicable. The certificate in respect of T.D.S. shall be issued by the Bank as per rate.  No claim whatsoever on this account shall be entertained.

8. QUANTITY OF WORK TO BE EXECUTED
The quantities shown in the schedule of quantities are intended to  cover the  entire  new  structure indicated in the drawings  but  the  Employer reserves  the  right to execute only a part or the whole  or  any  excess thereof without assigning any reason therefore. Variations in the value is however not expected to be more than + 25%.
9. OTHER PERSONS ENGAGED BY THE EMPLOYER
The employer reserves the right to execute any part of the work included in this contract or any work which is not included in this contract by other agency or persons and contractor shall allow all reasonable facilities and use of his scaffolding for the execution of such work. The main contractor shall extend all co-operations in this regard.
10. EARNEST MONEY 
The tenderer will have to deposit an amount of Eighty Five thousand only in the form of Bank draft drawn in favor of “Central Bank of India, GWALIOR” at the time of submission of tender as an Earnest Money. The employer is not liable to pay any interest on the Earnest Money. The Earnest Money of the unsuccessful tenderers will be refunded without any interest soon after the decision to award the work is taken or after the expiry of the validity period of the tender.

The retention amount will be refunded to the contractor fourteen days after the defect liability period, provided the contractor has satisfactorily carried out all the works and attended to all the defects in accordance with the conditions of contract.  No interest is allowed on Retention Money.
11. CONTRACTORS TO PROVIDE EVERYTHING NECESSARY
The contractor shall provide everything  necessary for the proper  execution  of  the work according to the intent and meaning of  the  drawings, schedule of quantities and specifications taken together whether the same may  or may not be particularly shown or described therein provided  that the same can reasonably be inferred there from &if the contractor finds any discrepancies therein, he shall immediately  & in writing refer  the same to the  Employer / Architect/ PMC whose decision shall be final  and  binding. The contractor shall provide him self for ground & fresh water for carrying out of the works at hi own cost. The Employer shall on no account be responsible for the expenses incurred by the contractor for hired ground or fresh water obtained from else where.
The rates quoted against individual items will be inclusive of everything necessary to complete the said items of work within the contemplation of the contract and beyond the unit price. No extra payments will be allowed for incidental or contingent work, labor and/or materials inclusive of all taxes and duties whatsoever except for specific taxes, if any, stipulated in the tender documents.

The contractor  shall supply, fix and maintain at his own cost  for  the execution  of any work, all tools tackles, machinery and  equipment's  and all  the necessary scaffolding, , watching and lighting  by night  as well as by day required not only for the proper  execution  and protection of the said work but also for the protection of the public and safety  of  any adjacent roads, streets, walls,  houses,  buildings,  all other  erections, matters and things and the contractor shall  take  down and  remove any or all such scaffolding, etc. as occasion shall be required or when ordered  to do  so  and shall fully reinstate  and make good all  matters  and  things distributed  during  the execution of works to the  satisfaction  of  the Employer/Architect.

The Contractor shall at all times give access to workers employer by the Architect / Employer or any men employed on the  buildings and  to  provide  such  parties with  proper sufficient  and  if required special scaffolding, hoists and ladders and provide them with water and lighting and leave or make any holes, grooves etc. in any work where directed by the employer as may be required  to enable such workmen to lay or fix pipes, electrical wiring, special fittings  etc. The quoted rates of the tenders shall accordingly include all these above mentioned contingent works.

12. TIME OF COMPLETION, EXTENSION OF TIME & PROGRESS CHART

1.
Time of completion: The entire work is to be completed in all respects within the stipulated period. The work shall deem to be commenced within seven days from the date of acceptance letter issued to the contractor or the day on which contractor is instructed to take possession of site, whichever is latter.  Time is the essence of the contract and shall be strictly observed by the contractor. 
The work shall not be considered as completed until the  Employer  have certified in writing that work has been completed and the defects liability period shall commence from the date of such certificate.

2.
Extension of Time : If, in the opinion of the Employer/Architect/ PMC the works be delayed,(a) By reason of any exceptionally inclement weather, or (b) by reason  of  instruction  from  the  employer in consequence  of  proceedings  taken  of threatened by or disputes, with adjoining or neighboring owners or (c) by the  works, or delay, of other contractors or tradesmen engaged or  nominated by the Employer and not referred to in the specification or (d)  By reason of authorized extra and additions or (e) By reason of any combination of workmen or strikes or lockout effecting any of the building trades or  (f)  From other causes which the employer may consider are beyond the control of the contractor, the Employer at the completion of the time allowed for the contract shall make fair and reasonable extension of the time for completion in respect therefore. In the event of the Employer failing to give possession of the site upon the day specified above the time of completion shall be extended suitably.

In case of such strikes or lockouts, as are referred to above, the contractor shall immediately give the employer, written notice thereof. Nevertheless,  the  contractor shall use his best endeavors all  that  to prevent  delay, and shall do all that may be reasonably required, to  the satisfaction  of the employer to proceed with the works and on his  doing so that it will be ground of consideration by the employer for an  extension  of time as above provided. The decision of the Employer as  to  the period  to the allowed for an extension of time for completion  hereunder (which  decision shall be final and binding on the contractor)  shall  be promulgated at the conclusion of such strike or lockout and the employer shall  then,  in the event of an extension being granted,  determine  and declare  the  final completion date. The provision in  clause  13,  with respect to payment of liquidated damages shall, in such case, be read and construed as if the extended date fixed by the employer were  substituted for and the damage shall be deducted accordingly.

3. Progress of work : During the period of construction  the contractor shall maintain  proportionate  progress  on  the basis of a programmed chart  submitted  by  the contractor  immediately before commencement of work and agreed to by  the employer/Architect. Contractor should also include planning for procurement for scarce material well in advance and reflect the same in the programmed chart so that there is no delay in completion of the project.

13. LIQUIDATED DAMAGES

Should   the   work  be  not  completed  to  the  satisfaction   of   the Employer/Architect within the stipulated period, the contractor shall  be bound  to pay to the employer a sum calculated as given below by  way  of liquidated  damages  and  not as penalty during which  the  work  remains un commenced or unfinished after the expiry of the completion date.

	a)
	For contracts having time for completion 6 months & Less.
	1.00% of the estimated amount shown in the tender per week subject to a ceiling of 10% of the accepted contracted sum.

	b)
	For contracts having time for completion exceeding 6 months but not exceeding 24 months.
	0.5% of the estimated amount shown in the tender per week subject to a ceiling of 7.5% of the accepted contracted sum but not exceeding the total S.D. of the contract.

	c)
	For contracts having time for completion in excess of 2 years (24 months).
	0.25% of the estimated amount shown in the tender per week subject to a ceiling of 5% of the accepted contracted sum but not exceeding the total S.D. of the contract.


14. TOOLS, STORAGE OF MATERIALS, PROTECTIVE WORKS & SITE OFFICE REQUIREMENTS

The contractor shall provide, fix up and maintain in an approved position proper  office  accommodation  for the  contractor's  representative  and staff,  which  offices shall be open at all reasonable hours  to  receive instruction, notices or communication and clear away on completion of the work and make good all work disturbed.

All drawings maintained on the site are to be carefully mounted on boards of appropriate size and covered with a coat of approved varnish. They are to be protected from ravages of termites, ants and other insects.

The contractor shall provide at site at his own cost all artificial light required for the work and to enable other contractors and subcontractors to complete the work within the specified time.

The Contractor shall provide a suitable temporary hut for the watchmen and clear away the same when no longer required and to provide all necessary attendants, lights etc. required.

The contractor shall arrange for temporary latrines for the use of  workers  and field staff and keep the same in a clean sanitary  condition  to the  satisfaction of the Public Health Authorities and shall  cause  such latrines  and soil to be cleared away whenever necessary and  shall  make good all the works disturbed by these conveniences.

Every precaution shall be taken by the contractor to prevent the breeding of mosquitoes on the works during the construction and all receptacles, cisterns, water tanks etc. used for the storage of water must be suitably protected against breeding of mosquitoes. The contractor shall indemnify the employer against any breach of rules in respect of anti-malarial measures.

The  contractor shall not fix or place any placards or  advertisement  of any  description or permit the same to be fixed or placed in or upon  any boarding,  gantry,  building structure other than those approved  by  the Employer.

Protective Measures

The contractor from the time of being placed in possession of the site must make suitable arrangements for watching, lighting and, protecting the work, the site and surrounding property by day, by night, on all days including Sundays and other holidays.

Contractor shall indemnify the employer against any possible damage to the building, roads, or member of the public in course of execution of the work.

The contractor shall provide necessary temporary enclosures, gates, entrance etc. for the protection of the work and materials and for altering and adopting the same as may be required and removing on completion of the works and making good all works disturbed.

Storage of materials
The  contractor  shall provide and maintain proper sheds for  the  proper storage  and  adequate protection of the materials etc., and  other  work that  may  be executed on the site including the tools and  materials  of subcontractors  and  remove same on completion.

Tools

All instruments like steel tape etc. which is found necessary for the works shall be provided by the contractor for due performance of the contract.

All measuring tapes shall be of steel and suitable scaffolding and ladders that may be require for safety taking measurements and shall be supplied by the contractor.

The  Mistree's  and  the supervisors on the works shall  carry  with  them always  a  one  meter or two meter steel tapes, a measuring  tape  of  30 meters, a spirit level, a plumb bob and a square and shall check the work to  see that work is being done according to the drawings and  specifications.  The  site engineer will use any or all measuring  instruments  or tools  belonging to the contractor as he chooses for checking  the  works executed or being executed on the contract.

The contractor should cover in his rates for making provisions for all reasonable facilities for the use of his scaffolding, tools and plants etc. by subcontractors for their work.

15.
NOTICE AND PATENTS OF APPROPRIATE AUTHORITY AND OWNERS
The Contractor shall confirm to the provisions or any acts of the  legislature relating to the work, and to the regulations and By-Laws of any authorities, and / or any water, lighting and other companies, and / or authorities with whose system the structures were proposed to have constructed and shall before making any variation from the drawings or specifications that may be associated to so confirm, give the Employer/Architects written notice, specify the variations proposed to be made and the reasons for making them and apply for instructions thereon. the Employer on receipt of such intimation shall give a decision with a reasonable time.

The Contractors shall arrange to give all notices required for by the said acts, regulations or By-laws to be given to any authority, and to pay to such authority or to any public officer all fees that may be properly chargeable in respect of the work and lodge the receipts with the Employer

The contractor shall indemnify the employer against all claims in respect of  patent  rights, royalties, damages to buildings, roads or  member  of public in course of execution of work and shall defend all actions  arising  from  such  claims and shall keep the employer  saved  harmless  and indemnified in all respects from such actions, costs and expenses.

16.
CLEARING SITE AND SETTING OUT WORKS

The contractor shall set out the works and shall be responsible for the true and perfect setting out of the work and for the correctness of the positions, levels, dimensions and alignment of all parts thereof. If at any time, any error shall appear during the progress of any parts of the works the contractor shall at his own expenses rectify such error, if called upon to the satisfaction of the employer. The contractor shall further set out the work to the alternative positions at the site until one is finally approved and the rates quoted in his tender should include for this and no extra on this account will be entertained.

17.
ACCESS
Any  authorized  representative of the Employer/Architect  shall  at  all reasonable  times have free access to the works and/or to the  workshops, factories  or  other places where materials are being  prepared  or  constructed for the work and also to any place where the materials are lying or  from  where they are being obtained, and the  contractor  shall  give every facility to the bank or their representatives necessary for inspection  and examination and test of the materials and  workmanship.  Except the representatives of the Employer, no person shall be allowed at any time without the written permission of the Employer.

18.
MATERIALS, WORKMANSHIP, SAMPLES, TESTING OF MATERIALS

All  the works specified and provided for in the specifications or  which may  be  required to be done in order to perform and  complete  any  part thereof  shall be executed in the best and most workman like manner  with materials  of  the best and approved quality of the respective  kinds  in accordance with the particulars contained in and implied by the  specifications  and  as represented by the drawings or according to  such  other additional particulars and instructions as may from time to time be given by  the Employer/Architect during the execution of the work, and  to  his entire satisfaction.

If required by the Employer/Architect the contractor shall have to  carry out  tests  on materials and workmanship in  approved  materials  testing laboratories  or as prescribed by the employer at his own cost  to  prove that  the materials etc. under test confirming to the relevant  IS  standards  or as specified in the specifications. The necessary charges for preparation of mould, (in case of concrete cube), transporting, testing etc.  shall have to be borne by the contractor. No extra payment on this account would in any case be entertained. 

All the materials (except where otherwise described) stores and equipment required for the full performance of the work under the contract must  be provided  through  normal  channels and must include  charge  for  import duties,  sales  taxes, octroi and other charges and must be the  best  of their  kind available and contractor/s must be entirely  responsible  for the proper and efficient carrying out of the work. The work must be done in the best workman like manner. Samples of all materials to be used must be   submitted to the Employer/Architect when so directed by   the Engineer/Architects and written approval from Employer/Architect must be obtained prior to placement of order. The approved samples shall be kept with the Employer till the completion of work.

Should the work be suspended by reason of rain, strike, lockouts or any other cause, the contractor shall take all precautions necessary for the protection of work and at his own expenses shall make good any damage arising from any of these causes.

The contractor shall cover up and protect from damage, from any cause, all new work and supply all temporary doors, protection to windows, and any other requisite protection for the execution of the work whether by himself or special tradesmen or subcontractor and any damage caused must be made good by the contractor at his own expenses.

19.
REMOVAL OF IMPROPER WORK
The Employer shall during the progress of the work have power to order in writing from time to time the removal from the work within such  reasonable  time  or times as may be specified in the order  of  any  materials which in the opinion of the Employer/Architect are not in accordance with specification or instructions, the substitution or proper re-execution of any  work executed with materials or workmanship not in  accordance  with the  drawings and specifications or instructions. In case the  contractor refuses  to  comply with the order the employer shall have the  power  to employ  and  pay other agencies to carry out the work  and  all  expenses consequent  thereon or incidental there to as certified by  the  employer shall be borne by the contractor or may be deducted from any money due to or  that  may become due to the contractor. No certificate which may be given by the Architects shall relieve the contractor from his liability in respect of unsound work or bad materials.

20.
SITE ENGINEER / PROJECT MANAGEMENT CONSULTANT
The term, "Site Engineer / PMC” shall mean the person / agencies appointed & paid by the Employer to superintend the work. The contractor shall afford the Site Engineer /PMC every facility and assistance for examining the works and materials   for checking and measuring work and materials.  The  Site Engineer/PMC  shall have no power to revoke,  alter,  enlarge  or  relax  any requirements  of the contractor or to sanction any day  work,  additions, alterations, deviations, or omissions or any extra work whatever,  except in so far as such authority may be specially conferred by a written order of the Employer.

The Site Engineer/PMC shall have power to give notice to the contractor or to his foreman of non approval of any work or materials and such work shall be suspended or the use of such materials shall be discontinued until the decision of the employer is obtained. The work will from time to time be examined by the Architects, Engineer from the premises department of the Employer and the Site Engineer if any. But such examination shall not in any way exonerate the contractor from the obligation to remedy defects  which maybe found to exist at any stage of the work or after  the  same  is complete ,Subject to the limitations of this clause the contractor shall take instructions only from the Architects/Employer or his representative.

21.
CONTRACTOR’S EMPLOYEES
The  Contractor shall employ technically qualified and  competent  supervisors  for  the work who shall be available (by turn)  through  out  the working   hours   to  receive  and  comply  with  instructions   of   the Employer/Architects. The contractor shall engage at least one experienced Engineer as site-in-charge for execution of the work.  The contractor shall employ in connections with the work persons having the appropriate skill or ability to perform their job efficiently.

The contractor shall employ local laborers on the work as far as possible.

No laborers below the age of sixteen years and who is not an Indian National shall be employed on the work.

Any laborer supplied by the contractor to be engaged on the work on day work basis either wholly or partly under the direct order or control of the Employer or his representative shall be deemed to be a person employed by the contractor.

The contractor shall comply with the provisions of all labour legislation’s including the requirements of:

a) The payment of Wages Act.

b) Employer's Liability Act.

c) Workmen's Compensation Act.

d) Contractor Labor (Regulation & Abolition) Act, 1970 and   Central Rules 1974.

e) Apprentices Act 1961.

f) Any other Act or enactment relating thereto and rules framed    there under from time to time.

The  contractor shall keep the Employer saved, harmless  and  indemnified against  claims if any of the workmen or any other person and  all  costs and  expenses as any be incurred by the Employer in connection  with  any claim that may be made by any workman or any other person.

The contractor shall comply at his own cost with the order of requirement of any Health Officer of the state or any local authority or of the Employer regarding the maintenance of proper environmental sanitation of the area where the contractor's laborers are housed or accommodated, for the prevention of small pox, cholera, plague, typhoid, malaria and other contagious diseases. The contractor shall provide maintain and  keep  in good  sanitary  condition  adequate sanitary  accommodation  and  provide facilities  for pure drinking water at all times for the use of  men  engaged on the works and shall remove and clear away the same on completion of  the works. Adequate precautions shall be taken by the contractor to prevent nuisance of any kind on the works or the lands adjoining the same.

The contractor shall arrange to provide first aid treatment to the laborers engaged on the works. He shall within 24 hours of the occurrence of any accident at or about the site or in connection with execution of the works, report such accident to the employer and also to the competent authority where such report is required by law.

22.
DISMISSAL OF WORKMEN
The contractor shall on the request of the employer immediately dismiss from works any person employed thereon by him who may in the opinion of the employer be unsuitable or incompetent or who may misconduct himself. Such discharges shall not be the basis of claim for compensation or damages against the Employer or any of their officers or employee.

23.
ASSIGNMENT
The whole of the works included in the contract shall be executed by  the contractor and the contractor shall not directly or indirectly  transfer, assign  or underlet the contract or any part, share or  interest  therein nor, shall take a new partner without written consent of the employer and no  subletting  shall  relieve the contractor from the  full  and  entire responsibility of the contract or from active superintendence of the work during their progress.

24.
DAMAGE TO PERSONS AND PROPERTY INSURANCE ETC.
The  contractor  shall  be responsible for all injury to  the  worker  or workmen or persons, or things and for all damages to the  project works, materials, equipments, structural and/or decorative part of  property which may arise from the operations or neglect of himself or of  any subcontractor or any of his or a subcontractor's employees whether such injury  or  damage arise from carelessness, accident or any  other  cause whatsoever  in any way connected with the carrying out of this  contract. The  clause shall be held to include inter alias any damage  to  buildings whether  immediately  adjacent  or otherwise and  any  damage  to  roads, streets,  foot paths or ways as well as damages caused to  the  buildings and the works forming the subject of this contract by rain, wind or other inclemency  of the weather. The contractor shall indemnify  the  employer and  hold  harmless in respect of all and any expenses arising  from  any such  injury or damages to persons or property as aforesaid and  also  in respect  of any claim made in respect of injury or damage under any  acts of compensation or damage consequent upon such claim.

The  contractor shall re-instate, rectify and remedy all damages of  every sort mentioned in this clause so as to deliver the whole of the  contract works  complete  and perfect in every respect and so as to make  good  or otherwise  satisfy all claims for damages to the property or  third  parties.

The contractor shall affect the insurance necessary and indemnify the employer entirely from all responsibility in this respect. The insurance must be placed with company approved by the employer and must be effected jointly in the name of the contractor and the employer and the policy lodged with the latter. The scope of insurance is to include damage or loss to the contract itself till this is made over in a complete state. Insurance is compulsory and must be affected for the very initial stage. The contractor shall also be responsible for anything which may be excluded from the damage to any property arising out of incidents, negligence or defective carrying out of this contract.

The  employer  shall  be at liberty and hereby empowered  to  deduct  the amount of any damages, compensations, costs, charges and expenses arising or accruing from or in respect of any such claim or damages from any sums including the total security deposit due or to become due to the contractor.

25.
INSURANCE
Unless otherwise instructed the contractor shall insure the works for all risk  (include fire, flood, earthquake & third party) of  the  contractor for total tender value and keep them insured until the virtual completion of  the  contract against any loss or damage of the material and  of  the project.  The insurance must be placed with a company approved by the Employer in the joint names of the Employer and the contractor for such amount and for any further sum if called to do so by the Employer. Further the premium of such sum being allowed, to the contractor, as an “authorized extra”. 
The contractor shall deposit the policy and receipt premium paid with the Employer within 21 (twenty one) days from the date of issue of work order unless otherwise instructed. In default of the contractor insuring as provided above the Employer on his behalf may so insure and may deduct the premiums paid from any money due, or which may become due to the contractor. The contractor shall as soon as the claim  under  the policy is settled or the work reinstate by Insurance Company should they elect  to  do so, proceed with due diligence with the completion  of  the works  in the same manner as though the fire has not occurred and in  all respects under the conditions of the contract. The Contractor in case of rebuilding or rein-statement after fire shall be entitled to extension of time for completion as the Employer may deem fit.

26.
ACCOUNTS RECEIPT & VOUCHERS
The contractor shall, upon the request of the employer furnish them  with all  the  invoices, accounts, receipts and other vouchers that  they  may require in connection with the works under this contract. If the contractor shall use materials less than what he is required under the contract, the value of the difference in the quantity of the materials he was required to use and that he actually used shall be deducted from his dues. The decision of the employer shall be final and binding on the contractor as to the amount of materials. The contractor is required to use for any work under this contract.

27.


Before taking any measurement of any work the site Engineer or a subordinate deputed by him shall give reasonable notice to the contractor.  If  the contractor fails to attend at the measurements  after  such notice or fails to countersign or to record the difference within a  week from the date of measurement in the manner required by the  Site Engineer then in any such event the measurements taken by the Site Engineer or  by the subordinate deputed by him as the case may be is final and binding on the  contractor  and the contractor  shall have no right to  dispute  the same.
28.
PAYMENTS

All Bills shall be prepared by the contractor in the form prescribed by the Employer/ Architects. Normally one interim bill shall be prepared each month subject to minimum value for interim certificate as dated in these documents. The bills in proper forms must be duly accompanied by detailed measurements in support of the quantities of work done & must show deductions from all previous payments, retention money, etc.

The Employer / Architect shall issue a certificate after the due scrutiny of the contractor’s bill stating the amount due to the contractor from the Employer & the contractor shall be entitled to payment thereof, within the period of honoring the certificates named in these documents. In case of delay due to some reasons in the processing of such bills for payment, an adhoc advance of 75% of the billed amount may be paid on the request of the contractor for the smooth progress of work.

The amount state in the interim certificate shall be the total value of work properly executed & 75% of the invoice value of material brought to site for permanent incorporation into the work up to the date of the bills less the amount to be retained by the employer as retention money vide clause 10 of these conditions & less installments previously paid under these conditions, provided that such certificates shall only include the value of said material & goods as & from such time as they are reasonably, properly & not prematurely brought to or placed adjacent to the work & then only if adequately protected against the weather or other causalities.

The Employer will deduct retention money as described in clause 10 of these conditions. The refund of retention money will be made as specified in the said clause.
If the Employer has supplied any materials or goods to the contractor, the cost of any such materials or goods will be progressively deducted from the amount due to the contractor in accordance with the quantities consumed in the work.
All interim payments shall be regarded as payments by way of advance against the final payment only & not as payments for the work actually done & completed, & shall not preclude the requiring of bad, unsound & imperfect or unskilled work to be removed & taken away & reconstructed, or re-erected or be considered as an admission of the due performance of the contract, or any part thereof in any respect or the accruing of any claim, nor shall, it conclude, determine or affect in any way the power of the Employer under these conditions or any of them as to the final  settlement & adjustment of the accounts or otherwise or in any other way vary or affect the contract. The final Bill shall be submitted by the contractor within one month of the date fixed for completion of the work or of the date of certificate of completion furnished by the site Engineer & payment shall be made within three months. 

29.
FINAL PAYMENTS
The final bill shall be accompanied by a certificate of completion from the Employer/ Architect. Payments of final bill shall be made after  deduction of Retention Money as specified in clause 10 of these  conditions, which sum  shall  be  refunded after the completion of  the  Defects  Liability Period after receiving the Employer’s / Architect's certificate that  the contractor has rectified all defects to the satisfaction of the  Employer /  Architects. The acceptance of payments of the final bill by the contractor would indicate that he will have no further claim in respect of the work executed.

30. VARIATION/DEVIATIONS
The price of all such additional items/ non tendered items will be worked out on the basis of rates quoted for similar items in the contract wherever existing or an engineering rate analysis based on prevalent fair price of labor, material & other components as required. The tender rates shall hold good for any increase or decrease in the tendered quantities up to variations of 25%. For variations beyond 25%, the rates for the respective items may be reviewed on mutually agreed terms.

31.
SUBSTITUTION
Should the contractor desire to substitute any materials and workmanship, he/they must obtain the approval of the Architect/Employer in writing for any such substitution well in advance. Materials designated  in  this specification  indefinitely by such terms as "Equal" or "other  approved" etc.,  specific approval of the Employer/Architect has to be obtained  in writing.

32.
PREPARATION OF BUILDING WORKS FOR OCCUPATION AND USE ON COMPLETION
The whole of the work will be thoroughly inspected by the contractor and deficiencies and defects put right. On completion of such inspection the contractor shall inform the employer that he has completed the work and it is ready for inspection.

On completion, the contractor shall clean all windows and doors including the cleaning and oiling, if necessary, of all hardware, inside and outside, all floors, staircases, and every part of the building.  He will leave the entire building neat and clean and ready for immediate occupation and to the satisfaction of the Bank.

33.
CLEARING SITE ON COMPLETION
On  completion of the works, the contractor shall clear away  and  remove from  the site all constructional plant, surplus materials,  rubbish  and temporary  works  of every kind and leave the whole of the site  and  the works  clean  and in a workmanlike condition to the satisfaction  of  the Employer / Architects.
The contractor shall make good at his own cost and to the satisfaction of the Employer all defects, shrinkages or other faults which may appear within 6 months after completion of the work. In  default,  the employer  may  employ and pay other persons to amend and make  good  such damages,  losses  and expenses consequent thereon or  incidental  thereto shall  be made good and borne by the contractor and such damages,  losses and  expenses  shall be recoverable from him by the employer  or  may  be deducted by the employer, in lieu of such amending and making good by the contractor, deduct from any money due to the contractor a sum  equivalent to the cost of amending such work and in the event of the amount retained being  insufficient,  recover that balance from the contractor  from  the amount retained under clause No. 10 together with any expenses the  Employer may have incurred in connection therewith.

34.
CONCEALED WORK
The  contractor  shall  give due notice to the  Employer / Architects whenever any work is to be buried in the earth, concrete or in the bodies of  walls or otherwise becoming inaccessible later on, in order that  the work may be inspected and correct dimensions taken before such burial, in default  whereof the same shall, at the option of the  Employer/Architect be  either  opened up for measurement at the contractor's expense  or  no payment may be made for such materials. Should any dispute or differences arise after the execution of any work as to measurements etc., or other  matters which cannot be conveniently tested or checked, the notes of the Employer / Architect shall be accepted as correct and binding on the contractor.

35.
ESCALATION

The rates quoted shall be firm throughout the tenure of the contract (including extension of time, if any, granted)& will not be subject to any fluctuation due to increase in cost of materials, labor, sales tax, octroi, GST etc. unless specifically provided in these documents.

The price variation clause being adopted by the RBI may be followed, if such a situation arises on a case to case basis. 
Further in case of variation in the wages of labor due to statutory enactments like the revision of the Minimum Wages Act by more than 10%, the increase in actual cost due to implementation of the statutory provision based on the number & category of labor actually borne on the Muster during the period under consideration may also be considered, if provided in the tender. 
36.
IDLE LABOUR
Whatever the reasons may be no claim for idle labor, additional establishment cost of hire and labor charges of tools and plants would be entertained under any circumstances.

37.
SUSPENSIONS
If the contractor, except on account of any legal  restraint  upon  the Employer preventing the continuance of the work, abandons, suspends  work or  in the opinion of the Employer, the contractor neglects or  fails  to proceed  with  due diligence in the performance of his part of  the  contract, the Employer shall have the power to give notice in writing to the contractor requiring the work be proceeded within a reasonable manner and with reasonable dispatch, such notices purport to be a notice under  this clause.

After  such notice shall have been given the contractor shall not  be  at liberty to remove from the site of the works or from any ground  contiguous  thereto  any  plant or materials to subsist from the  date  of  such notice being given until the notice shall have been complied with. If the contractor shall fail for 7 (seven) days after such notice has been given to proceed with the works as therein prescribed, the Employer may proceed as provided in clauses 38 (Termination of contract by Employer).

38.
TERMINATION OF CONTRACT BY EMPLOYER
If the  contractor being a company go into liquidation whether voluntary  or compulsory  or  being a firm shall be dissolved or  being  an  individual shall be adjudicated insolvent or shall make an assignment or a  composition  for the benefit of  the greater part, in numbers or amount  of  his creditors  or shall enters into a Deed or arrangement with his  creditors or if the official assignee in insolvency of the receiver of the contractor in insolvency, shall repudiate the contract, or if a receiver of  the contractor's   appointed by court shall be unable, within  fourteen  days after  notice  to him requiring him to do so, to show to  the  reasonable satisfaction  of the Employer  that he is able to carry out  and  fulfill the  contract,  and  if so required by the employer  to  give  reasonable security  therefore,  or if the contractor shall suffer  execution  to  be issued, or shall suffer any payment under this contract to be attached by  or  on  behalf of and the creditors of the contractor,  or  shall  assign charge or encumber this contract or any payments due or which may  become due  to the contractor there under, or shall neglect  or fail  to  observe and perform all or any of the acts matters of things by this contract  to be observed and performed by the contractor within three clear days after the notice shall have been given to the contractor in manner  hereinafter mentioned   requiring  the contractor to observe or perform the  same  or shall use improper materials or workmanship in carrying on the works,  or shall in the opinion of the employer not exercised such due diligence and make  such due progress as would enable the work to be  completed  within due  time agreed upon, and shall fail to proceed to the  satisfaction  of the employer after three clear days notice requiring the contractor so to do  shall have been given to the contractor as hereinafter mentioned,  or shall  abandon the contract, then and in any of the said cases, the  bank may  not withstanding previous waiver determine the contract by a  notice in  writing to the effect as hereinafter mentioned, but  without  thereby effecting  the powers of the employer of the obligations and  liabilities of the contractor the whole of which shall continue in force as fully  as if  the contract, had not been so determined and as if the  works  subsequently  executed had been executed by  or on behalf of  the  contractor (without thereby creating any trust in favor of the contractor). Further the  employer or his agent, or servants, may enter upon and take  possession  of the work and all plants, tools, scaffolding,  sheds,  machinery, steam  and other power utensils and materials lying upon premises or  the adjoining  lands  or roads and sell the same as his own property  or  may employ  the same by means of his own servants and workmen in carrying  on and  completing the works or by employing any other contractors or  other persons  or person to complete the works and the contractor shall not  in any  way  interrupt or do any act, matter of thing to prevent  or  hinder such other contractors or other persons or person employed from  completing  and finishing or using the materials and plants for the  works  when the  works shall be completed, or as soon thereafter as conveniently  may be, the employer shall give notice in writing to the contractor to remove his surplus materials and plants and should the contractor fail to do  so within  a period of fourteen days after receipt by him. The employer may sell the same by Public Auction and shall give credit to the contractor for the amount so released. Any expenses or losses incurred by  the  employer  in  getting the works carried out by other contractors  shall  be adjusted  against the amount payable to the contractor by way of  selling his  tools and plants or due on account of work carried out by  the  contractor  prior  to  engaging other contractors or  against  the  Security Deposit.

39.
ARBITRATION
All  disputes  or differences of any kind whatsoever which shall  at  any time arise between the parties hereto touching or concerning the works or the  execution  or  maintenance thereof of this contract  or  the  rights touching or concerning the works or the execution of maintenance  thereof of this contract or the construction remaining operation or effect thereof or to the rights or liabilities of the parties or arising out of or in relation  thereto  whether during or after determination for  closure  or Breach of the contract (other than those in respect of which the decision of  any  person is by the contract expressed to the  final  and  binding) shall  after written notice by either party to the contract to the  other of them and to the Employer hereinafter mentioned be referred for adjudication to a sole arbitrator to be appointed as hereinafter provided.

For the purpose of appointing the sole Arbitrator referred to above,  the employer  will send within thirty days of receipt of the notice,  to  the contractor  a  panel  of three names of persons who  shall  be  presently unconnected with the Organization for which the work is executed.

The Contractor shall on receipt of the names as aforesaid, select any one of the persons named to be appointed as a sole Arbitrator and communicate his name to the employer within thirty days of receipt of the names.  The employer shall thereupon without any delay appoint the said person as the Sole Arbitrator. If the contractor fails to communicate such selection as provided above within the period specified, the component authority shall make the selection and appoint the selected person as the Sole Arbitrator.

If the Employer fails to send to the contractor the panel of three names as aforesaid within the period specified, the contractor shall send   to the employer a panel of three names of persons who shall all be unconnected with either party. The Employer shall on receipt of the names as aforesaid select any one of the persons named and get appointed him as a Sole Arbitrator. If the Employer fails to select the person and  appoint him  as  the Sole Arbitrator within 30 days of receipt of the  panel  and inform  the contractor accordingly, the contractor shall be  entitled  to appoint  one  of  the person from the panel as the  Sole  Arbitrator  and communicate his name to the Employer.

If the Arbitrator so appointed is unable or unwilling to act or resign his appointment or vacates his office due to any reason whatsoever another Sole Arbitrator shall be appointed as aforesaid.

The work under the contract shall however continue during the Arbitration proceedings and no payments due or payable to the contractor shall be withheld on account of such proceedings.

The Arbitrator shall be deemed to have entered on the reference on the date he issues notice to both the parties fixing the date of the first hearing.

The Arbitrator may from time to time with the consent of the parties enlarge the time for making and publishing the award.

The Arbitrator shall give a separate award in respect of each dispute or difference referred to him. The Arbitrator shall decide each dispute in accordance with the terms of the contract and give a reasoned award.  The venue of Arbitration shall be such place as may be fixed by the Arbitrator on his sole discretion.

The fees, if any, of the Arbitrator shall, if required to be paid before the award is made and published, be paid half and half by each of the parties. The costs of the reference and of the award including the  fees, if  any, of the Arbitrator who may direct to and by whom in  what  manner such  costs or any part thereof shall be paid and may fix or  settle  the amount of costs to be so paid.

The award to the Arbitrator shall be final and binding on both the parties.

Subject  to aforesaid the provisions of the Arbitration Act 1940  or  any statutory modification or reenactment thereof and the rules made  there under  and  for the time being enforce, shall apply  to  the  Arbitration proceeding under this clause.

The  Employer  and contractor hereby also agree  that  arbitration  under clause  shall be a condition precedent to any right to action  under  the contract  with  regard to the matters hereby expressly agreed  to  be  so referred to arbitration.

SECTION III
SPECIAL CONDITION OF CONTRACT

1.
 MATERIALS PROVIDED BY EMPLOYER
i)The  Employer may reserve to themselves the right to  provide  certain materials  as mentioned for the work at the time of awarding contract  or during  the progress of the work and these shall be jointly inspected  by the  Engineer and the contractor before issue of  materials.  Suitability and sufficiency of the material shall be checked by the contractor.

ii) After the materials are received, the contractor shall not decline to accept responsibility for the proper quality, safety and sufficiency of the resulting work or structure by alleging defects of materials received from the Employer.

iii)The  value of materials provided by the Employer shall be  calculated at  the prevalent market rates/invoice rates including all taxes,  duties transportation,  labor  and other incidentals by the  Engineer  and  the amounts shall be deducted in full from the interim Bill of the contractor as and where applicable.

iv)  For all materials, issued free of cost to the contractor, the rates for such complete, items shall be suitably modified/varied by the Engineer, unless otherwise provided for in the contract.

v) Wastage of extra quantity of materials used by the contractor over and above the allowed quantity as determined by the Engineer shall be taken as unnecessary and unauthorized and such use/wastage shall be at the cost of the contractor.

The Employer will not be bound to take back such materials found  surplus with  the contractor either before or after the completion of work or  on an earlier termination of the contract, unless otherwise provided for  in the contract.

vi) On loss or damage of any such materials, it shall be replaced by the contractor with the same quality/brand with the approval of Engineer or the value of such material would be recovered from interim bill of the contractor at the prevalent market rate, as would be appropriate in the opinion of the Engineer.

1.2(i) The contractor will be required to pay all taxes levied by the Central and/or State Governments on such part of his profit in respect of the contract as in chargeable therewith under the laws for the time being in force.

1.2(ii) The contractor's staff will be liable to pay all taxes levied by the Central and/or Union Governments on such of their salaries as are chargeable there with under the laws for the time being in force and the contractor shall conform such duties in regard to the deduction thereof as may be lawfully imposed on him.

1.2(iii)
Contractor shall have to produce the certificate from the manufacturer or their authorized dealers for all procured products confirming use of specific materials at site. 

2.
ELECTRICITY AND WATER

2.1
The Contractor shall be provided Electricity and water at one point only by the Bank and the Contractor shall pay to the Bank for the consumption of this facility on mutually agreed upon by the Bank and the Contractor.

2.2 Regarding all factory made products for which I.S.I. marked products are available, only products bearing I.S.I. marks shall be used in the work unless otherwise mentioned in the list of approved make of material in the tender. 

2.3 CARE FOR EXISTING PROPERTY: The Contractor shall make all necessary arrangements as required by the Employer to ensure that all existing property of the Owner are not damaged or disrupted by the Contractor in any way.  If in spite of his best efforts there is some disruption, or lose occurs, the Contractor shall reinstate and make it good as early as possible without any additional cost to the Owner.

3.
DRAWINGS: Some of the detailed drawings may not be ready at the time of placing the order.  The Contractor will have to proceed with the work till such time such drawings are released.    The Contractor shall have absolutely no claim on the Owner on this account. Efforts will be made however, to release drawings progressively to have un-interrupted progress. Contractor will prepare/Shop drawings wherever required by Bank/Architects. 

SECTION IV

MEASUREMENT

1.
 MEASUREMENT

1.1
The number of pages for measurements alone shall be 100 per book. If convenient, the measurement book may be provided with perforated sheets, in triplicate, for dispatch to concerned authorities. The pages shall be serially machine numbered. The book shall be in the custody of the Site Engineer.

1.2 
In addition to pages for measurements, pages shall be provided for index. Instructions, Certificate of Condition (wholeness) of the Book and Record of handling and taking over.

1.3
Each book shall bear an identifying number.

2.
RECORDING OF MEASUREMENTS
2.1
The measurements shall be generally recorded by the Site Engineer or by the Consultant of the bank, specifically authorized for the purpose.

2.2
The Site Engineer (or his representative) shall take joint measurements (i.e. accompanied by the contractor's authorized representative) of the work as it progresses and record them directly in the Measurement Books.

2.3
It shall be ensured that the method of measurement is in accordance with the contract. The precision in measurements shall be as laid down in IS   1200. Any points of disagreement with the contractor pertaining to measurements shall be promptly referred to the decision of the competent authority.

2.4
Extra/deviated items, as claimed by the contractor, shall not be recorded in Measurement Book until they are approved by the competent authority.

2.5
In  case some allegedly extra/deviated item is carried  out  by  the contractor while complying with approved drawings and specifications, and the same is to be covered up, the Site Engineer shall check the item  and its specification and record its measurements but simultaneously enter up the  provision  that their admittance is subject to the approval  by  the competent  authority. Both the measurements and the proviso shall be got signed by the contractor.

2.6
The measurement Book shall not be handed over to the contractor at any time. The contractor or his representative may be permitted by the Site Engineer to see it in his presence and/or make a (concurrent) copy of his own. The contractor shall, however, be warned that his copy shall be regarded as an unofficial copy of the bank's Measurement Book. This is the only authorized document in the matter.

2.7
The measurement shall be signed at the end of each session on measurement of the day's work, as the case may be, by both the parties (i.e. Measurer/Site Engineer and the contractor).

3.
CONCEALED WORK
3.1
The contractor shall give due notice to the Employer whenever any work is to  be covered up in the bodies of walls or  otherwise,  becoming  inaccessible  later on, in order that the  work  may  be inspected  and  correct dimensions taken before such burial.  In default where of the same shall, at the opinion of the Employer be either opened up for measurement at the contractor's expenses or no payment may be made for such materials. Should any dispute or difference arise after the execution of any work as to measurements etc. or other matters which cannot be conveniently tested or checked, the notes of the employer shall be accepted as correct and binding on the contractor.

4.
The following instructions shall be borne in mind while taking measurements.

4.1
The work shall be measured in the same sequence as constructed.

5.
Checking of Measurements: Checking of the measurements shall be as under.
5.1
It shall not be perfunctory and should result in revealing errors, accidental or deliberate, by the staff.  It should also serve as a process of instruction to junior staff:

5.2 Measurements recorded shall be checked not less than 25% by Bank’s representative from the Zonal Office and 100% measurement by the architect. 

SECTION V

SAFETY CODE

SCAFFOLDS

1.
 Suitable  scaffolds shall be provided for workmen for all  works  that cannot safely be done from the ground, or from solid construction  except in  the case of short duration work which can be done "safely  from  ladders"  when  a  ladder is used, it shall be of  rigid  construction  made either  of  good quality wood or steel. The steps shall  have  a  minimum width of 450 mm and a maximum rise of 300 mm. Suitable hand hold of  good quality wood or steel shall be provided and the ladder shall be given  an inclination not steeper than 1/4 to 1 (1/4 horizontal and 1 vertical).

2.
Scaffolding or staging more than 4m, above the ground floor, swung or suspended  from  an overhead support or erected with  stationary  support shall  have  a guard rail properly bolted, braced or  otherwise  secured, at least  1 m, above the floor or platform of such scaffolding or  staging and  extending  along the entire length of the outside and  ends  thereof with  only such openings as may be necessary for the delivery of  materials.  Such scaffolding or staging shall be so fastened as to prevent it from swaying from the building or structure.

3.
 Working  platforms, gangways and stairway shall be  so  constructed that  they do not sag unduly or unequally and if the height of the  platform,  gangway or stairway is more than 4 m, above ground level or  floor level, they shall be closely boarded and shall have adequate width and be suitably fenced as described in (ii) above.

4.
Every opening in the floor of a building or in a working platform shall be provided with suitable means to prevent the fall of persons or materials by providing suitable fencing or railing whose minimum height shall be 1m.

Where ever there are open excavations in ground, they shall be fenced off by suitable railing and danger signals installed at night so as to prevent persons slipping into the excavations.

5.
Safe means of access shall be provided to all working places. Every ladder shall be securely fixed. No portable single ladder shall be over 9M, in length while the width between side rails in rung ladder shall in no case, be less then 290 mm, for ladder up to and including 3M, in length for longer ladders this width shall be increased at least 20 mm for each additional meter of length.

6.
A sketch of the ladders and scaffolds proposed to be used shall be prepared and approval of the Engineer obtained prior to construction.

OTHER SAFETY MEASURES

7.
All personnel of the Contractor working with in the plant site shall be provided with safety helmets. All welders shall wear welding goggles while doing welding work and all metal workers shall be provided with safety gloves. Persons employed on metal cutting and grinding shall wear safety glasses.

8. Adequate precautions shall be taken to prevent danger from electrical equipment.  No materials on any of the sites of work shall be so stacked or placed as to cause danger or inconvenience to any person or the public.

9. The contractor shall take all the measures on the site of the work to protect the public from accidents & shall be bound to bear the expenses of defense of every suit, action or other proceedings at law that may be brought by any person for injury sustained owing o neglect of the above precaution & to pay any such persons or which may with the consent of the contractor, be paid to compromise any claim by any such person.
PERSONAL SAFETY EQUIPMENTS

10.
 All necessary personal safety equipment as considered adequate by the Engineer should be kept available for used of the person employed on the site and maintained in a condition 
suitable for immediate use, and the Contractor should take adequate steps to ensure proper use of equipment by those concerned.

a)
Workers employed on mixing asphalt materials, cement and lime mortars shall be provided with protective footwear and protective goggles.

b)
Those engaged in white washing and mixing or stacking or cement begs or any materials which are injurious to the eyes shall be provided with protective goggles.    

c)
Those engaged in welding works shall be provided with welder’s protective eye sights lids.

d)
When workers are employed in sewers and manholes, which are in use, the Contractor shall ensure that the manhole covers are opened and are ventilated at least for an hour before the workers are allowed to get into manholes so opened shall be cordoned off with suitable railing and provided with warning signals or boards to prevent accident to the public.

e)
The Contractor shall not employ men below the age of 18 years and women on the work of painting with products containing lead in any form. Wherever men above the age of 18 years are employed on the work of lead painting, the following precaution should be taken:

i) No paint containing led or led products shall be used except in the form of paste or ready made paint.

ii) Suitable face masks should be supplied for use by the  workers when  paint is applied in the form of spray or a  surface  having lead paint dry rubbed and scrapped.

iii) Overalls shall be supplied by the Contractor to the workman and adequate facilities shall be provided, to unable the working painters during the execution of work.

11.
The safety provisions should be brought to the notice of all concerned by display on a notice board at a prominent place at work spot. The person responsible for compliance of the safety code shall be named therein by the contractor.
SECTION VI
MODEL RULES FOR THE PROTECTION OF HEALTH

AND SANITARY ARRANGEMENTS FOR WORKERS

DEFINITION
1.a) 'Work Place' means a place at which, at an average 50 workers  are employed in connection with construction work.

FIRST AID
2.(a) At every work place, they shall be maintained in readily  accessible place first aid appliance including an adequate supply of  sterilized dressings and sterilized cotton wool. The appliance shall be kept in good order and in large work place they shall be placed under the charge of a responsible person who shall be readily available during working hours.

DRINKING WATER
3.a)
In every work place, there shall be provided and maintained at suitable places easily accessible to labor sufficient supply of cold water fit for drinking.

b)
Where drinking water is obtained from an intermittent public water supply, each work place shall be provided with storage where such drinking water shall be stored.

c)
Every water supply of storage shall be at a distance of not less than 15 m, from any latrine, drain or other source of pollution.  Where water has to be drawn from an existing well which is within the proximity of latrine, drain or any other source of pollution, the well shall be properly chlorinated before water is drawn from it for drinking. All such wells shall be entirely closed in and be provided with a trap door which shall be dust and water proof.
SECTION –VII
PREAMBLE TO BILL OF QUANTITIES
RATES TO INCLUDE:

Rates quoted shall be for the items completed in all respect at all floors/heights/levels including all taxes, octroi and the cost of all materials, fittings, fixtures, all labor and for all the operations as detailed in the specifications and contract conditions. Apart from other factors mentioned in the specifications and contract conditions, rates quoted for the items in this schedule shall also include the following:

1.
GENERAL:
a. Whether mentioned or not in the Bill of Quantities, all works are to be carried out as per the drawings, designs, catalogues and or instructions of the Architects/Bank.  extra shall be paid over the quoted rates for not understanding the designs etc. before hand.

b. Sample of all works/items shall be got approved from the Architects/Bank before taking the mass production in hand and nothing shall be paid for the cost of samples.

c. Any incidental work required to complete the item and not specifically covered in the item as mentioned in Bill of Quantities shall be completed at no extra cost.

d. Unless otherwise specified all exposed surfaces of wood/wooden moldings and plywood of loose furniture/items tops shall be finished in at least two coats of melamine polish, including staining to match the shades of laminates etc.

e. All laminates for furniture items shall be 1.0 mm thick for vertical & 1.5 mm for hoz. Spaces, in Satin finish, color texture and shade as per the schemes given by the Bank/Architect.  

f. Unless otherwise specified, all inner surfaces, sides and under sides of furniture items, drawers/cabinets shall be polished/Painted flat oil painted as directed by Architects.

g. All exposed edges of plywood/block boards shall be finished with teak wood lip pings 5 mm thick of profile as per detail and Melamine polished unless otherwise specified and no extra cost shall be paid.

h. All furniture items shall be delivered at site packed in polythene sheets.

2. WOOD WORKS:

a. Wherever ply is mentioned it will mean ply wood.

b. All Board/Ply will be of BWP/BWR Commercial Type.

c. All teak wood will mean CP. teak.

3.
HARDWARE:
3.1 Necessary handles, tower bolts, ball catchers, stoppers, hinges, brass/GI screws, nails, locks, sliding rails, nut and bolts etc. shall be provided by the Contractor which shall be out of the approved make of these materials annexed in the technical specifications/approved by Architects/Bank.

4.
PAINTING AND POLISHING:
4.1 All finishes, shade of colors, texture of fabrics including all surfaces of finishes like POP, painting, lamination, paneling, stitching joints in upholstery, all polishing shall be as per the satisfaction of the Architects/Bank.

4.2 Thoroughly brushing the surface to be finished, free from mortar dropping and other foreign matter including preparing the surface and sand papering to give an even surface.

4.3 For painting and polishing items – on all kinds of wood and wood based surfaces.

4.4 All painting work to be completed with at least one coat of the primer along with two coats of the paint as per the Technical Specification, Manufacturer’s specification and to the satisfaction of the Architects/Bank.

4.5 All the polishing works to be completed with at least two coats of the polish of the approved make as pr the list of approved manufacturers and to the full satisfaction of the Architects/Bank.

5.
GLASS WORKS:
5.1 The edges of glass tops for tables wherever shown shall be beveled as per approval of the Architects.

6.
PARTITIONS AND PANELLING
a. Quoted rate shall include labor/materials required to fix the sub-frame to the wall with MS flats (‘L’/ ‘U’) shape clamp with adequate screws and repairing the portion damaged while putting the gut ties. etc. and  making good the same.

b. Quoted rate shall be inclusive of making provisions for electrical conduits and switch boxes and time required while coordinating with other Contractors for the final finishing of the work.  

c. The partition frame work shall be provided up to the RCC slabs at top but measurement for payment shall be of partition up to false ceiling and frame /support of partition above false ceiling shall be carried out within the quoted rate for which no extra shall be paid.

d. All work/materials will be as per good engineering practice.

e. Wherever glass is mentioned it will be clear float glass.

SECTION - VIII
SPECIFICATIONS

1.
 GENERAL: 

1.1
This section of the specifications covers all general civil work is any, for which no separate detailed specifications have been included.

1.2
All these works shall be done in accordance with the drawings and instructions for the Engineer-in-charge. Unless otherwise so specifically mentioned, the latest CPWD Specifications (New Delhi) for the particular item of work shall be followed.   In case of any dispute regarding the intent of the specifications, the Engineer’s decision shall be final.

All work shall be done as per approved drawings, specifications, site instructions and with specified materials/makes as approved.   In case the Contractor desires to substitute an approved/specified material/make with an alternative one he must get specific approval of the same before its use in the work.    Failure to do so will make the work liable to rejection irrespective of the fact that it might not have been detected and rejected earlier.

1.3
All finished work must be truly vertical and horizontal or in any other plane as shown and required and true to lines and levels. The Tenderers must inspect the various existing surfaces and areas on which he has work on and take whatever measures necessary to achieve  the above objective and include the cost of the same in his rates as no extra will be payable for this purpose.

1.4
Samples of all items of work shall be prepared & got approved before proceeding with the work. For partitions complete layout shall be marked on the floor at the site for inspection & checking; only after approval installation shall commence.

1.5
Teak wood used anywhere in the work shall be Ist quality Teak wood. If anything to the contrary is mentioned elsewhere in these documents or drawings the above shall prevail & Tenderer shall be deemed to have quoted their rates accordingly.

2.
WOOD WORK AND JOINERY:

2.1 
PLY WOOD: Ply wood shall be BWR as per IS-303-1975 Specifications 

2.2
BLOCK BOARDS: Block board shall be as per IS: 1659-1979 BWR grade. 

2.3
FLUSH DOORS:
2202 Pt I (1991) Specification for wooden flush door shutter (cellular and

hollow core type) ply wood face panels BWR grade.
2.3
LAMINATE: Laminates where specified shall be of approved brand type, texture and thickness and manufacturer as per IS: 2046-1969.Fixing of laminates shall be done as per best trade practices and strictly as per printed instructions of the manufacturers using phenol Formaldehyde Synthetic Resin adhesive of approved make. Unless otherwise indicated laminated shall be 1.0 & 1.5 mm thick of approved make.

2.4
JOINERY:All details shall conform to the drawings, but all measurements shall be checked at site.   The scantlings shall be accurately planned and finished smooth to hold full dimensions shown in the drawings after finishing and rebates, rounding and moldings made before they are framed.   No patching or plugging of any kind shall be prepared and got approved by the Engineer before proceeding with bulk manufacture.

 3.
IRONMONGERY:

3.1
This section shall cover all finish hardware, latches, locks and other fittings and fixtures etc., used in wood doors.   All finish hardware shall be well made, reasonably smooth, and free sharp edges and corners flaws and other defects and shall be as per relevant Indian Standard Code.   Unless otherwise required all finish hardware shall be polished brass.

3.2
All hardware shall be of approved make and shall be specifically got approved by the Engineer before ordering.   No fittings and fixtures shall be fixed before all major work is over.   While fixing correct handling of fixtures shall be ensured.

LIST OF APPROVED MAKE OF A C C E P T A B L E    MATERIALS

ENTIRE MATERIAL LISTED BELOW SHOULD BE FIRST APPROVED BY THE BANK AND CONSULTANT BEFORE EXECUTING)
	 S. No.
	Item
	Specified Material

	1
	False Ceiling-
	 

	
	1)Gypsum Board
	1). 12.5mm thick Gypsum Board of Gypsum India Ltd.  with sections of 26 gauge GI sheet of “Gypsum India Ltd.” Company.

	
	2)Armstrong Tiles
	2). Armstrong 600x600x(12-18 mm thick) perforated tiles as per “Armstrong Pvt. Ltd.” company’s specifications.

	2
	Aluminum Sections
	16-18 Gauge anodized Aluminum tubular sections with 20 micron (black) of 50x50mm, 50x40mm for partition and 16-18 gauge anodized Aluminum sections of 40x115mm for bottom rail & top rails of doors, 40x150mm lock rail and 40x20mm plain for shutters of the sliding window.  or equivalent.

	
	 
	All aluminum section to be anodized in black shade and shall be of “Jindal/Nalco/ Hindalco. 

	
	1.Partition
	 

	
	2.Door
	 

	3
	Aluminum Grill      
	Aluminum grill of 8- 10 mm dia. rod with 75x75mm mesh DG 202 of “Jindal/Nalco/Hindalco .

	4
	MDF/Particle Board
	12 mm thick both side laminated “Greenlam /Duro /Century.” with Ivory/ Beige shade BSL, Interior grade IS: 12823.

	5
	1.Plywood/ Block Board (BWP/BWR)
	1)      Phenol bonded, water proof, plywood of all required thickness (6mm,9mm,12mm,19mm and 25mm) of  “Century, Duro, Greenply.”  conforming to IS: 303, IS: 710 & IS:1659 

	
	Laminates
	GreenLam / Sunmica / Formica 

	6
	Wood
	Well-seasoned teak-wood 

	7
	Moulding & Lipping
	1st Quality Teak Wood.

	8
	Wood Preservative
	“ASIAN/ NEROLAC/ BERGER/ICI/ DULUX.”

	9
	Adhesive  
	“FEVICOL (SH)/ PIDILITE or equivalent.”

	10
	Glass
	Plain float glass “Modi  / Saint Gobain.”   of all thickness                               

	11
	Lock/Night Latches    
	“GODREJ/ LINK/HARRISON.”

	12
	Hydraulic Door closer
	“DORMA, GODREJ.” confirming to IS:3564:1986

	13
	Floor Spring (Double action 100 kg. -150 kg)
	“GODREJ, DORMA.”  confirming to IS: 6315:1992 & IS:7197:1972

	14
	Drawer Channel/ Slider   (Telescopic)
	Sleek computer keyboard slide of required length mounting telescopic, steel ball slider STDS series keyboard of “EBCO, HETTICH, GODREJ.”.

	15
	Key Board Drawer/Tray    
	Ready to use, computer keyboard tray KBT series keyboard of “EBCO, HETTICH, GODREJ.”

	16
	Hard ware   
	All the necessary hardware shall be of ISI marked with best quality/ and as per Bank’s approval.

	17
	Teak wood    
	Beading and Moulding to be of first quality teak wood.

	18
	Paint 
	1. Acrylic paint/ Luster Paint: - “ROYALE, ICI, ASIAN DULUX/NEROLAC.” 

	
	Off white, Desert White, Cream
	2. Oil bound distemper:-  “ROYALE, ICI, ASIAN DULUX/NEROLAC.” 

	
	 
	3. Synthetic Enamel Paint: - “ROYALE, ICI, ASIAN DULUX/NEROLAC.” 

	
	 
	4. Texture Paint: - “WEATHER COAT, EXTERIOR, APEX, SNOCEM, ASIAN.” 

	19
	Flooring
	1.      Vitrified tiles: - 600x600x (8-10 mm thick) Premium Range   “NITCO/ MARBONITE/ JOHNSON.”

	
	(Off white)
	2.     Ceramic Tiles:-“NITCO/ MARBONITE / JOHNSON.”

	
	 
	3.      Vinyl Flooring:- 2mm thick “Rikwin, ARMSTRONG, Marblex.”

	20
	Roller /Venetian Blinds (Off white, Abstract Biege B/O-0002   
	“VISTA, MAC, AUROLUX.”.

	21
	Chairs with fabric 
	“GODREJ, FEATHERLITE, WIPRO.” (High, Mid, Low back and visitors chairs)  

	22
	Visitors Seating    
	Chrome plated Perforated seats OF ABOVE BRANDS

	
	
	3seater  and  2seater 

	23
	Rubber/ Polyurethane /Tapestry/Leather Foam    
	Foam of all thickness of 40-50 density HD U- Foam of “Dunlop, MM, TATA.”.

	
	
	

	24
	Wash Basin   
	Vitreous China, conforming to IS: 2556 “Hindware /Cera /Johnson /Parryware.”.

	25
	WC (EWC/Orissa Pan)
	Vitreous china, conforming to IS:2556  “HINDWARE/CERA/JOHNSON/PARRYWARE.”.

	26
	GI Pipes
	“C”- Class GI pipes, for all the diameters, “JINDAL, BINDAL, TATA.” 

	27
	Tap & Flush cock   
	CP Finish bib cock and pillar cock, flush cock. “PLUMBER, JENITH, JAL, JAGUAR, MAC,BELL.”

	28
	Sink
	Stainless steel sink. “NIRALI.” 

	29
	Cement
	Best quality, 53 Grade (OPC)- “ACC, AMBUJA, BINANI, BIRLA. confirming to IS:1489-1976

	30
	Steel
	Hot rolled deformed bars confirming to IS:1139-1966 (Fe-415 HYSD)  “TATA, Jindal, Rathi SAIL, RINL”

	31
	Aggregates  
	Aggregates shall comply with the requirements of IS:383-1970

	32
	Brick Works        
	All brick work shall confirm to IS:2212-1962

	33
	Reinforcement Bending and Fixing Works  
	Bending and fixing of bars for concrete works shall be as per IS:2502-2009

	
	
	

	34
	RCC/PCC Works  
	All RCC/PCC works shall confirm to IS:456-2000

	35
	Aluminum Composite Panel    
	“Alstone / Alucobond /Eurobond.” 

	36
	Modular Work Stations/Table
	“Godrej, Wipro, Featherlite.”


ELECTRICAL:
	S. No.
	Items
	Make
	Code

	1
	MCCBs, MCBs, ELCBS, RCCBs, DB, ICTPN, TP, HRC fuse, Change over switch, Switch Fuse Unit
	L&T, Legrand, Siemens 
	IS: 8828 for MCB 

IS:13947 for MCCB

IS:12640 for RCCB

IS:13703 for HRC fuse

IS:13947 for SFU

	2
	FRLS insulated Elect. Wires Sheathed/ unsheathed, Flexible LT cable, Multi core/single core Cable, Flat cable for submersible pumps
	Polycab, RR 
	IS: 694 for PVC cable

1.1 KV GRADE-FRLS

	3
	Rotary Switches. Selector Switches
	L&T, GE, ABB, Siemens 
	Relevant IS 



	4
	Exhaust fan ,Pedestal fans, Ceiling fan
	Crompton, Orient, Usha 
	IS: 374 for ceiling fan

IS: 2312 for Exhaust fan

	5
	Electronic Energy Meter
	L&T, HPL, ABB 
	IS:13779/1999

	6
	Central Air Conditioning Plants , Package type plant ,Window/Split AC, Cassette type AC
	Toshiba, Hitachi, Mistibushi 
	*Only 3 star and above rating in Window/Split/Cassette/HAT AC

	7
	Electrical accessories Modular -switch, Plugs sockets, ceiling rose, Angle holder, holders
	Crabtree, MK, Legrand
	IS: 3854 for switches

IS: 1293 for plugs& sockets

IS: 371 for ceiling rose

IS: 1258 for lamp holder Bakelite

	8
	Bell Buzzer
	 Anchor, Cona, Leader 
	IS:2268



	9
	Electronic fan regulator
	Crabtree, MK, Legrand 
	IS:11037

	10
	PVC Conduit pipe & Casing -capping for electrical wiring
	AKG, Setia, BEC (ISI) 2 mm thick 
	IS:9537/93

	11
	Current Transformer
	Siemens, L&T, Schneider 
	IS: 2705 

	12
	Relays 


	Siemens, L&T, ,ABB, BHEL, GE 
	IS: 3231/65



	13
	Data Cable
	D Link.
	(With 15 years certification)

	14
	Light Fittings
	LED – Philips 
	

	15
	Telephone Cable
	Delton, Polycab 
	(Conductor dia – 0.61 sqmm)

	16
	Industrial Socket with box
	 MDS Legrand – 32 amp / Hager L&T 
	

	17
	Changeover Switches
	Havells – On Load (Euro Load) 
	

	18
	Panel Board
	16 swg CRCA sheet steel 
	Fabricated and vermin proof and dust proof with necessary stiffners  with indicators of Telemechenique / L&T and Input/Output Volt & Ampere Meter


Seal & Signature 

of Firm,

· No Deviation permissible. Wherever Contractor proposes to use “other” makes (i.e. Other than specified) the same shall be done only after prior approval from the Bank’s Civil/Electrical Engineer.
SPECIFICATION OF WORKMANSHIP : -
1) All the exposed surfaces (that come in first sight or in direct vision) such as top/ front/ sides of counter, table etc. shall be covered with laminates/ tapes/border.
2) All the hidden exposed surfaces (that does not come in first sight or in direct vision) shall be finished with 0.8 mm thick laminate of Green lam/ Sunmica/ Formica and there shall be no putty, primer or any oil bonded synthetic enamel paint in these areas.
3) All the exposed edges and corners of plywood of 12mm & 18mm shall be protected by nailing wooden beads/border of required size.

4) All the wooden beading/batons shall be finished with high-class sprit polish in natural shade.

5) All the exposed edges and corners of furniture shall be comfortably and smoothly chamfered/ rounded off to avoid any sharp and pointed ends.

6) A good surface preparation shall be done prior to applying primer/putty/paint/polish either on walls, ceiling or on furniture.

7) All the finishing shall be done with due care & perfection so that final quality/look/appearance/glare/shine achieved is of the required standard and satisfaction. 
8) All the operative units/members of items, fixed hardware/ fittings/ fixture etc. such as locks, levers, hinges, door closures, latches etc. shall be adequately smooth and well in operation/performance at the time of handing over work/site to the Bank.
ANNEXURE- I

TECHNICAL BID
(Information to be furnished by the applicants)
	1
	Name of the organization
	

	2
	Registered Office Details
(Submit firm registration certificate)
	Postal address
	

	
	
	Telephone nos


	

	
	
	E-mail address
	

	3
	Financial Strength- Average Annual Turnover & Profit in Rs.
	

	
	(Submit attested copy of ITR, Balance sheet attached by Charted Accountant )
	
	Turnover (in Rs.)
	Profit (in Rs.)

	
	
	FY 2014-15:
	
	

	
	
	FY 2015:16:
	
	

	
	
	FY 2016-17:
	
	

	4
	Details of similar work executed:


	

	
	(Submit completion certificate of similar works mentioned in eligibility criteria with details in separate sheet)
	
	Works
	Place of work
	Amount

	
	
	1
	
	
	

	
	
	2
	
	
	

	
	
	3
	
	
	

	5
	PAN Number (Submit copy of PAN)
	

	6
	TIN Number (Submit copy of TIN)
	

	7
	Service Tax Number (Submit copy of Service Tax Registration)
	

	8
	ESI/EPF registration Number (Submit copy of ESI/EPF Registration)
	

	9
	Solvency Certificate (Submit Solvency certificate)
	Yes / No       of Amount Rs. ………………...


DECLARATION:

 I/We hereby submit the information in your prescribed proforma and understand that if any information is found to be false at a later date, contract / order made between us and Central Bank of India will be treated as invalid. I/We agree that the decision of Central Bank of India in selection will be final and binding on me/us. All the information furnished in the attached sheets is correct to the best of my/our knowledge. Bank shall have the authority to verify all the information provided by me/us. All supporting documents shall be provided by me/us in authenticity of the information furnished. I/We agree that I/We have no objection if inspection of my/our premises/workshop, shop etc. is done by the officials of the Bank. 

Place:  








     Signature:

Date: 







Name & designation:

 





Organization:
[image: image6.emf]
ANNEXURE- II

FINANCIAL BID

Abstract Sheet for Works at proposed Regional Office GWALIOR

[image: image7.emf]:: Rs   Abstract Sheet for Refurbishing of UCO Bank; BO: BHIND:                    ABSTRACT SHE ET       1.   INTERIOR FURNISHING :                             Rs …………………………………………….     2.   ELECTRICAL &  other works :                        Rs…………………………………………….       TOTAL incl. all applicable taxes: Rs……………  …………… (in figures)     (………………………………………………………………………………………………)(in words )                                                                  


Seal & Signature 

of Firm,

	B.O.Q. for  R.O. (INTERIOR FURNISHING WORK PART-I)

	S.No.
	Item/Description
	Quantity
	Unit
	Rate
	Amount

	1. CIVIL /FAÇADE WORKS 

	a
	ACP CLADDING: Design, Supply, Fabrication and installation / Fixing of Aluminum Composite Panels of approved make for external cladding and canopy cladding in combination of solid / Metallic colours, including all necessary frame work and complete weather sealing. The composite panel should consist of 3 mm LDPE sandwiched between 2 skins of 0.5mm thick Aluminum sheet making a total panel thickness of 4 mm.  The supporting framework shall be made to suit the grid requirement at site out of extruded section 38x38x3mm aluminum angle section or 50x25x1.6mm tube section running vertically or horizontally fixed to building structure through M.S clamps prefixed to masonry with suitable anchor fastener or screws as required after aligning the framework for level and lines. the ACP panel cut to size and bent at edges to form a tray to be fixed to aluminium grid tubes cleats, angles etc with metal screws. All hardware will be corrosion resistant. The gaps will be sealed using weather sealant like Dow Corning 789 or any other approved brand. Note: the external surface shall be well protected with self-adhesive peel off masking foil which is to be peeled off after the completion of all the works.
	           160.00 
	Sqft.
	
	

	 
	 
	 
	 
	 
	 

	b.
	GRANITE CLADDING / FLOORING : Providing and fixing 19 mm thk  finished granite slabs of colour as approved fixed with 20 mm thk cement mortar 1:4 mix (1 part cement, 4 parts coarse sand) as per the drawing. The grooves to be as/drg & instruction of architect incharge and slabs to be in perfect line, level and plumb. Joints to be filled with cement based matching grout .Basic Rate of granite - 200/- per sq.ft (For Entry Steps/ Facade)
	             20.00 
	Sqft.
	
	

	c
	Pantry/Storage Platform: Providing and fixing polished and half round moulded edge 18 mm thick (of any colour) Granite slab (Basic rate Rs.200/- sqft) on the CC 3'' thick pantry/storage platform of any shape (triangular/straight/rectangular) complete with cleaning of joints and curing. The measurement will be of actual stone area.
	             30.00 
	sq.ft
	
	

	 
	 
	 
	 
	 
	 

	d
	Providing & fixing SS sink of size min 450 x 450mm.
	               1.00 
	LS
	
	

	 
	 
	 
	 
	
	

	e
	Plumbing for Sink with two nos of SS taps and UPVC pipes including all necessary materials.
	               1.00 
	LS
	
	

	 
	 
	 
	 
	TOTAL=
	      

	 

	2
	FALSE CEILING WORKS (Measurements shall be taken of the plan area only)
	 
	 
	 
	 

	a
	GYPSUM BOARD CEILING: Providing and fixing suspended false ceiling in STRAIGHT OR CURVED shape with COVE design consisting of 12.5mm thick Gypsum  board ( India Gypsum)  suspended on GI framework. GI framework to consist of GI perimeter channels 0.55mm thick 20mm x 30mm along perimeter of false ceiling of ceiling, screw fixed to wall/partition with nylon sleeves and screws @ 600mm c/c. Suspending GI intermediate channels of size 0.9mm thick 45mm x 15mm from the soffit at max dist 1220mm c/c with ceiling angle 0.55mm thick 25mm x 10mm fixed to soffit using proprietary supplied GI cleats and steel expansion fasteners. Boards to be finished with proprietary supplied jointing tape and jointing compound and sand papered to achieve a smooth and seamless finish and 2 coats of primer along with coats of Acrylic paint suitable  for Gypsum board upto Bank's Satisfaction .Rate quoted to include all vertical drops , overhang, projection all cut-outs required for light fixtures, smoke detectors and other services cut-outs complete as directed by Architect. 
	        1,800.00 
	Sqft.
	
	

	 
	 
	 
	 
	 
	 

	b
	GRID FALSE CEILING /Modular False ceiling :Providing and fixing suspended false ceiling consisting : approved make MODULAR CEILING
	        2,350.00 
	Sqft.
	
	

	
	Tile: Classic Lite RH 99 Bevelled Tegular;
	
	
	
	

	
	Suspension system: Silhouette type 15mm wide
	
	
	
	

	
	Horizontal plane measurements are to be inclusive of all vertical drops, edge mouldings, fascias, etc. Rate quoted to include all cut-outs required for light fixtures, smoke detectors and other services cut-outs complete as directed by Architect. Rate quoted to include cost of providing support framework formed of perimeter channels for fixing light fixtures, AC grills/diffusers etc. Also to provide concealed perimeter channel support as required supporting modular grid ceiling sections at junction between gypboard false ceiling and modular grid tile ceiling.
	
	
	
	

	 
	 
	 
	 
	 
	 

	c
	TRAP DOORS: Providing and fixing trap doors for access to the areas above false ceiling. The trap door shall have an external frame made of 2"x2" in good quality seasoned wood scantling on which the shutter is hinged. Shutter shall be made of 19 mm. BWP ply. The exposed side shall be laminated in approved quality and colour. Concealed heavy duty hinges shall be used to mount the shutters and locking shall be provided with panel locks. The shutter shall be moulded in level with the false ceiling forming a groove all around. Sufficient number of hinges and locks shall be provided to avoid sagging of the shutter. Key also shall be supplied. No extra rate shall be provided for suspenders or frame works all round for linking the trap door to gypboard false ceiling.
	           200.00 
	Sqft.
	
	

	 
	 
	 
	 
	Total=
	

	 

	3
	PAINTING WORKS
	 
	 
	 
	 

	a
	INTERNAL PAINTING. (FOR WALLS & CEILING)
	        4,000.00 
	Sqft.
	
	

	
	Providing and applying premium acrylic emulsion paint of interior grade of Approved brand and of approved shade firstly removing old paint with scratching using stiff wire / fiber brush, sand paper, fine steel wool then removing all loose and powdery residue, any fungus and algae thorough brushing, cleaning, making surface imperfections such as holes, dents, small visible cracks by filling using mixture and then after surface preparations, then applying one coat of  approved primer, then providing and applying two coats of  premium acrylic emulsion paint of approved colour, shade. Complete as per the direction of Consulting Engineer in-charge.                                                                                               
	
	
	
	

	 
	 
	 
	 
	 
	 

	b
	ENAMEL PAINT: Painting with synthetic enamel/ oil paint of approved brand and colour to give and even shade in two or more coats as required/ directed. The cost includes making the surface smooth with oil based putty, red oxide paint in one coat in case of iron steel grill etc. complete after surface preparation rubbing cleaning complete. Door, Window, Grills, CG, Shutters.
	        1,500.00 
	Sqft.
	
	

	 
	 
	 
	 
	 
	 

	c
	WALL PAPER: Providing & Installing of wall paper as per approved samples having 20% recycled content by weight minimum 10% post-consumer, and meets or exceeds all type-II requirements of CCC-W- 408A/D and industry voluntary standard CFFA-w- 101A/D. Weight of minimum 20 to 13.3 oz/ly (619 to 452gms/sqm) & having a minimum width of 52 to 54". Backing of Osnaburg or approved equivalent, Fire safety norms as per Class A (ASTM E-84) Tunnel Test, Corner burn test as per NFPA 286 & Life safety code NFPA 101. All material & adhesive shall be free from Lead, Mercury, Cadmium & chromium & have anti-microbial features. (Note: No extras will be paid for overlapping & wastages or any additional material required for installation) (Basic cost of Wall Paper Up to: Rs.60 per sqft FOR site)
	           400.00 
	Sqft.
	
	

	 
	 
	 
	 
	 
	 

	d
	PUNNING -This item including providing and applying Plaster of Paris punning of required 12 mm thickness over existing wall & ceiling surfaces in true level and plumb complete as directed.  
	           250.00 
	Sqft.
	
	

	 
	 
	 
	 
	Total=
	      

	 

	4
	INTERIOR FURNISHING WORKS
	 
	 
	 
	 

	a
	P/F SOLID/PARTLY GLAZED PARTITIONS made out of Aluminum cross section   size  2"x1 1/2" of framework 2'-0" c/c both ways , covered with 8 mm thk BWR/BWP grade ply wood / partly glazed with approved shape & shade  1mm thk laminate/mica fixing on inside of panel with 1.5 mm thk grooves in panel as per the design with provision of the openings in the panel for switch boards, box and cuts in frame for carrying conduits if necessary and fixing 1.0 mm laminate on the outside face of shade and colour as per Bank’s colour scheme given in the tender specification with 8 mm TOUGHENED glass to be provided as given in the design.                                                                  The open edges are to be blocked by teak wood bead with polish of required size and design. All provisions to be made for all electrical, networking boxes onto partition framework at required heights/levels with necessary additional supports as directed.
	        2,025.00 
	Sqft.
	
	

	 
	 
	 
	 
	 
	 

	b
	FULL HEIGHT 12MM THK. TOUGHEN GLASS PARTITION: P/F 12 mm thick glass full height glass embedded in aluminum anodized sections all around for external facade glazing. Anodizing to be Natural Finish shade. (on special cases, subject to approval).(Frame work details as mentioned in item no. 1) The works includes fixing of glass with Top & Bottom surfaces with proper support/frame.
	           275.00 
	Sqft.
	
	

	 
	 
	 
	 
	
	

	c
	Providing and fixing of frameless toughen glass doors with below fixtures of size 900x 2100mm
	               3.00 
	Nos
	
	

	
	Door Lock
	 
	 
	 
	 

	
	Door stopper
	 
	 
	 
	 

	
	Floor Machine
	 
	 
	 
	 

	
	Parch fitting
	 
	 
	 
	 

	
	S.S. Handle 12'' long
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 

	d
	Flush Door: Providing and fixing single leaf solid core flush door 40mm thick factory made, finished on both sides with 1.0mm thick laminate of approved shade as indicated in drawing. Shutter to be lipped on all sides with 12mm thick teak wood beading. Applicable hardwares to be considered for following doors according to requirement as per detailed drawings including below mentioned hardware-Door closer, SS Ball bearing Hinges, SS foot operated Door stopper, SS Mortise Latch Lock / concealed dead lock, SS Mortise Handle.
	 
	 
	 
	 

	
	Size of door 900 x2100
	4.00
	Nos
	
	

	
	Size of door 600 x2100
	4.00
	Nos
	
	

	 
	 
	 
	 
	 
	 

	e
	Providing and fixing PVC door for toilets All necessary fitting should be used, material is of approved brand. Size of door 750 x2100 with 30 mm thickness. (Make: Sintex or equivalent)
	               6.00 
	Nos
	
	

	 
	 
	 
	 
	
	

	f
	WALL PANELLING: Fabricating and fixing wall/column paneling to consist of 37.5mm x 50mm Aluminum Sections at spacing not exceeding 600mm both ways (horizontal and vertical).  Paneling framework to be secured to wall surface/column surface. Paneling framework to be clad on one side with 8mm thick BWR/BWP grade ply finished with 1.0mm thk laminate including skirting of 100mm high & 1.5 mm x 1.5 mm groove at skirting level
	           600.00 
	Sqft.
	
	

	 
	Laminated Box Paneling: Providing and fixing Laminate finished wooden Box paneling over existing columns consisting of 12mm thick Flexi Ply cold presses with 1.0 mm thick laminate of approved make & shade over Aluminum/wooden sections framework in design and pattern as per drawings. The panels shall have grooves of 7.5 mm x 7.5 mm at corners with 6 mm thk wooden lipping around the grooves / or SS laminate as per drawing. The panels and the groove shall be sprit polished and finished with melamine matt coating to an even shade as per the approval of the EIC. Basic rate of laminate: Rs. 60 per sqft FOR site.
	           600.00 
	Sqft.
	
	

	 
	 
	 
	 
	
	

	g
	WOODEN BOX: Rolling shutter boxing made up in 19mm thk Marine plywood laminated / Exterior grade Bison Panel frame painted as per Architects approval. Measurement to be considered for all four sides.
	             40.00 
	Sqft.
	
	

	 
	 
	 
	 
	 
	 

	h
	FILE STORAGE CABINETS: Providing and fixing the 1'-9" wide storage units. The storage units shall have shutters made in 19mm BWR/BWP grade plywood and finished in laminate of approved shade including top. The storage units shall have intermediate shelves made in 19mm thick plywood with matching wood lipping. The storage shall have matching wood edge moulding as per the detail drawings. This also includes providing necessary hardware like handles, hinges, locks, tower bolts etc. of approved make. All exposed wooden surfaces shall be stained to shade. (same for Over Head storage/Low ht. storage required above Pantry counter.)
	 
	 
	 
	 

	 
	Low ht. storage units
	    500.00 
	Sqft.
	
	

	 
	Overhead storage units
	    150.00 
	Sqft.
	
	

	 
	Full ht. storages units
	1,400.00 
	Sqft.
	
	

	 
	 
	 
	 
	
	

	i
	FROSTED FILM: Providing and pasting frosted film (3M, Garware make) on glass work including Bank’s logo as required & as directed by the architect.
	300.00 
	Sqft.
	
	

	 
	 
	 
	 
	
	

	j
	Vertical Blinds: P/F Blinds made using 100% polyester with acrylic polymer coating. (only for external windows. In case of front facia necessary approval need to be obtained). Weight-390gm/sqm, Degree of opacity-100%, Light Fastness-4/6. Make: MAC/VISTA/HUNTER DOUGLAS
	           400.00 
	Sqft.
	
	

	 
	 
	 
	 
	
	

	k
	Rolling BLINDS -P/F Blinds made using 100% polyester with acrylic polymer coating.(only for external windows. In case of front facia necessary approval need to be obtained). Weight-390gm/sqm, Degree of opacity-100%, Light Fastness-4/6. Make: MAC/VISTA/HUNTER DOUGLAS
	           300.00 
	Sqft.
	
	

	 
	 
	 
	 
	 
	 

	l
	Zebra Blinds- P/F Blinds made using 100% polyester with acrylic polymer coating.(only for external windows. In case of front facia necessary approval need to be obtained). Weight-390gm/sqm, Degree of opacity-100%, Light Fastness-4/6. Make: MAC/VISTA/HUNTER DOUGLAS
	           175.00 
	Sqft.
	
	

	 
	 
	 
	 
	
	

	m
	NOTICE/PIN UP BOARD: Providing and fixing notice board of 6mm ply backing fixed on a frame of 50 mm x 25 mm well-seasoned Teak/Sal wood polished all around. 12mm thk. soft board cladded with fabric of matching colour fixed over ply with teak wood beading and shade complete with all fixtures necessary as required. Basic cost of fabric is Rs. 50 /sqft.
	           180.00 
	Sqft.
	
	

	 
	 
	 
	 
	 
	 


Magnetic WHITE BOARD with Duster: Providing and fixing of magnetic white board of approved make scratch resistant matt finish P3 surface consisting of ceramic steel of thickness 0.55mm to 0.65 mm, having a weight of 3-4 kgs per sqm. The core material shall be of interior grade 9mm thickness with density 700 to 800 kg/cum. With a backing of galvanized steel of 0.25 mm thickness having approximate weight of 1.96

kgs/sqm. This entire assembly shall be housed in an anodized aluminum extruded section conforming to IS-6477 and IS-3965/2673 and corners of moulded ABS. The front and back surface will be affixed with 10-15 micron silver matt satin finish. This should be provided with clamp for hanging arrangement with locking facility including one set of accessories comprising of magnets, magnetic dry markers and magnetic

	 erasers. Size: 3' x 4' (900mm x 1200mm)
	               2.00 
	Nos.
	
	
	

	 
	 
	 
	 
	 
	 

	o
	ARTIFICIAL PLANTERS & PLANTER BOX: Providing & fixing of 1'-6" x 1'-6" planter box 18" high, made of 19mm thick marine ply board, with teak wood Gola of size 1½ ”x ¾ ” as per design, which is to be polished as per color scheme. The planter box shall be finished with 1mm thick laminate of approved shade / colour, complete as per Bank’s approved brand/make. Inside of planters shall be finished with thin sheet of aluminum. Planter box to be furnished with white rounded pebbles & Artificial Bamboo Silk trees or Artificial Palm Trees of 3'-0" ht. 
	             16.00 
	Nos.
	
	

	 
	 
	 
	 
	 
	 

	p
	Automatic Glass Doors: Providing and placing automated glass doors with system
	 
	 
	 
	 

	 
	Providing & fixing Automatic sliding door system of ht 2200 mm with front mounted Automatic runner of length 2400 mm so as to provide clear passage gap of 1200 mm to have 2 individual runner mounted 12 mm clear toughened glass sliding shutters. Automatic system to be of DORMA ES-200. Easy automatic bi parting sliding door operator, modular design i/c Microprocessor control, self-learning with adjustable parameters for opening & closing speed, hold open time & opening & closing force, reversing when obstruction is en-countered. Class of protection IP 20. The system to made operative only on UPS power supply 230v,50/60Hz. Operator length 2400 mm with shutter opening passage of 1200 mm with clear min ht of 2050 mm. Max. Weight per leaf = 2 x 85 Kg (for Bi-parting doors). Operator body finish: Silver Anodized finish. Accessories light Barriers, pair of radars, Battery pack floor guide etc all complete with fixing of operator & glass by authorised DORMA agency. System to include 5 years warranty on motors & 1 year on accessories. 
	               1.00 
	set
	
	

	 
	 
	 
	 
	 Total= 
	

	 

	5
	P & F OF  FURNITURE ITEMS
	 
	 
	 
	 

	a
	Side Table: Providing and placing the Modular corner/side table of approved make & model of size 600(W)x600(D)x505(H) with 8mm thick tempered glass top and SS understructure connected with top glass via SS frame. Load bearing capacity is 15kg complete in all respect.
	
	
	
	

	
	Equivalent Model: Featherlite make 'CENTRE TABLES' series 'VERVE GLASS 610 FS' model.
	 4.00 
	Nos.
	
	

	 
	 
	 
	 
	
	

	b
	Centre Table: Providing and placing the Modular center table of approved make & model of required size with 8mm thick tempered glass top and SS understructure connected with top glass via SS frame. Load bearing capacity is 35kg complete in all respect.
	 
	 
	
	

	
	Equivalent Model: Featherlite make 'CENTRE TABLES' series 'VERVE GLASS 610 FL' model. size 1200(W)x600(D)x425(H)
	               1.00 
	Nos.
	
	

	
	Equivalent Model: Featherlite make 'CENTRE TABLES' series 'PARKWELL' model. Size: 900mm dia. x 450(H)
	               1.00 
	Nos.
	
	

	 
	Equivalent Model: Featherlite make 'CENTRE TABLES' series 'PARKWELL' model. Size: 600mm dia. x 450(H)
	               1.00 
	Nos.
	
	

	 
	 
	 
	 
	 
	 

	c
	REVOLVING CHAIRS: P&F of high back revolving chair of approved make & model with following specifications: Seat size shall be 480mm(W)x470mm(D), Back size shall be 470mm (W)x580mm(D) and chair size shall be 720mm(W)x720mm(D)x910-1000mm(H) Seat Height: 425-515mm. The seat is made up of 1.2cm thk. hot presses plywood upholstered with fabric and moulded Polyretahane foam. The back is a fabricated tubular frame. assembly: powder coated and upholstered with a fire retardant mesh type 100% High Tenacity Polyester fabric. The back tubular frame is made of Dia. 1.9cm x 0.16cm thk. M.S.E.R.W tube. The polyrethane foam for seat is moulded with density =45 kg/m3 and hardness =20 on Hampdon machine at 25% compression. The back cover is a perforated strip fabricated from 0.08cm thk CR steel and powder coated. The seat is covered on the underside with black polypropylene non-woven fabric. The armrest top is injected molded from black Polypropylene and mounted on to a fixed M.S. tubular arm rest support. The support can be statically adjusted ±1.5cm, vertically 360 degree revolving type. Single point control, Front pivot for tilt with feet resting covered with a black Polypropylene molded 2 piece hubcap at the center. 
	 
	 
	 
	 

	
	SRM: Equivalent Model: Featherlite make 'OFFICE CHAIR' series 'ASTRO HB' model.
	               1.00 
	Nos.
	
	

	
	DRM/CM: Equivalent Model: Featherlite make 'OFFICE CHAIR' series 'ASTRO MB' model.
	               5.00 
	Nos.
	
	

	
	OFFICER/SWO: Equivalent Model: Featherlite make 'OFFICE CHAIR' series 'Smart Mesh Revolving' model.
	             31.00 
	Nos.
	
	

	
	Conference room Chairs: Equivalent Model: Featherlite make 'OFFICE CHAIR' series 'Contact Project MB fixed arms' model.
	             20.00 
	Nos.
	
	

	 
	 
	 
	 
	
	

	d
	 SOFAS: Providing & placing Sofa of approved make & model in synthetic leather. The frame should be tropical seasoned Hardwood/SS and particle board. Seat and back foam should be of 35 D. Polyurethane slab stock foam with 25mm recron layer. Leg should be made of MDF wooden Fascia with melamine coating or of SS complete in all respect.
	 
	 
	 
	 

	
	 3 Seater Sofas: Size: 1800(W)x710(D)x780(H)mm. Equivalent Model: Featherlite make 'SOFAS' series 'Indulge S 906E' model.
	               6.00 
	Nos.
	
	

	
	Single Seater Sofas: Size 770(W)x710(D)x780(H)mm. Equivalent Model: Featherlite make 'SOFAS' series 'Indulge S 906E' model.
	               2.00 
	Nos.
	
	

	 
	 
	 
	 
	 
	 

	e
	VISITOR CHAIRS: P&F of  visitor chair of approved make & model with following specifications: Seat size shall be 480mm(W)x470mm(D), Back size shall be 470mm (W)x580mm(D) and chair size shall be 720mm(W)x720mm(D)x910-1000mm(H) Seat Height: 425-515mm. The seat is made up of 1.2cm thk. hot presses plywood upholstered with fabric and molded Polyurethane foam. The back is a fabricated tubular frame. Assembly: powder coated and upholstered with a fire retardant mesh type 100% High Tenacity Polyester fabric. The back tubular frame is made of Dia. 1.9cm x 0.16cm thk. M.S.E.R.W tube. The polyurethane foam for seat is molded with density =45 kg/m3 and hardness =20 on Hampdon machine at 25% compression. The back cover is a perforated strip fabricated from 0.08cm thk. CR steel and powder coated. The seat is covered on the underside with black polypropylene non-woven fabric. The armrest top is injected molded from black Polypropylene and mounted on to a fixed M.S. tubular arm rest support. 
	 
	 
	 
	 

	
	SRM Cabin Visitor Chairs: Equivalent Model: Featherlite make 'OFFICE CHAIR' series 'Astro Visitor' model.
	               4.00 
	Nos.
	
	

	
	DRM/CM Visitor Chairs: Equivalent Model: Featherlite make 'OFFICE CHAIR' series 'Contact Project visitor ' model.
	             15.00 
	Nos.
	
	

	
	CONFERENCE Back chairs:  Equivalent Model: Featherlite make 'OFFICE CHAIR' series 'Smart Mesh visitor-without arms ' model.
	             60.00 
	Nos.
	
	

	
	OFFICER/SWO Visitor Chairs: Equivalent Model: Featherlite make 'OFFICE CHAIR' series 'Smart Mesh visitor ' model.
	             40.00 
	Nos.
	
	

	 
	 
	 
	 
	 
	 

	f
	Pantry/Dining Table: Providing and fixing modular dining Table of approved make & model. Table understructure is foldable and stackable, made with combination of Aluminum and plastic. Centre column is of serrated aluminum extrusion of diameter 70mm, which is anodized min. 25 microns. The base of table is made in 2 pieces of die cast aluminum with buffed finish. It is bolted together with the centre column and top flanges as/manufacturer specifications. Top size: 800mm x 800mmx1.2mm thick over 24mm thick (±1 mm) - Top assembly. Top made from MDF PU Coated.  welded stiffner assembly made from 0.6mm thick SS-304 sheet glued with top with special glue as/manfd. Specifications complete in all respect. Hieght from ground: 720 mm.
	 
	 
	 
	 

	
	Equivalent Model: Featherlite make 'CAFÉFOLD' series “CF-SQ-C-800” model.
	               3.00 
	Nos.
	
	

	 
	 
	 
	 
	
	

	g
	Pantry/Canteen Chair: Providing and placing Dining chair of approved make & model of size 520mmWx545mmDx805mm H. Seat Height 430mm, Seat and back shell is injection molded in Polypropylene of approved colours such as Red, Blue or green as approved. Tubular frame is in 19mm Dia stainlesss steel tube-304/J4 grade, complete in all respect.
	 
	 
	
	

	
	Equivalent Model: Featherlite make 'CAFETERIA' series 'Fressco' model.
	             10.00 
	Nos.
	
	

	 
	 
	 
	 
	 
	 

	h
	Meeting/Discussion Room Table: P&F Modular 4 seater conference table of approved make & model of circular size of dia. 1200mm.  Work surface 32mm thick (±1mm). Base material 18+12mm MDF board Laminate 1.0 mm on Top surface 0.6mm balancing laminate on bottom surface Chamfer edges PU matt melamine polished veneer of approved shade.  Base material 6mm plain particle board post laminated with 0.6mm Top laminate on either side 2mm thk and 0.8mm thk PVC edge bending of matching colour on outer edges of cross member. Legs made from 1.6mm Matt silver Anodized Aluminum extrusion. Legs assembled together with a plastic glide holder at bottom and 5mm thick MS powder coated sheet at top. The wire carrying is facilated through the hollow space between two legs extrusions and the wires are concealed between removable rigid PVC extrusion in the leg Access Flap and Switch mounting Tray made from Matt silver Anodized Aluminum extrusion and plastic molded components to facilitate.
	 
	 
	 
	 

	
	Equivalent Model: Godrej make 'CONFERENCE TABLE' series 'talk pod round-laminate top' model four seater.
	1
	Nos
	
	

	 
	 
	 
	 
	 
	 

	i
	CABIN TABLE with mobile pedestal, side(SRU) & back unit (HDU):
	 
	 
	 
	 

	 
	Modular Table: Providing & placing/fixing the modular main table of approved make & model of required size. 
	 
	 
	 
	 

	 
	Top: 25mm thick plain particle board (PPB) clad with 0.6mm thick post formed laminate and 1 mm thick backing laminate (BDL). Flat edge duly sealed with 2 mm thk PVC beading.
	 
	 
	 
	 

	 
	Side & Front Modesty: 18mm thk PPB clad with 1.0mm thk decorative laminate on both sides. Edge sealed with 2 mm thk PVC beading.
	 
	 
	 
	 

	 
	Mobile Pedestal: Providing and placing/fixing the modular mobile pedestal of approved make & model of required size, the drawer top shall be made out of 25mm thick MFC Board and all other panel made out of 18mm thick MFC board and the drawer fronts having metal Handle, central Lock & Castors of approved make with fittings, complete in all respect.
	 
	 
	 
	 

	 
	Side return Unit: Providing and palcing the modular side return unit of approved make & model of required size. The top, side & doors, partitions, shelves specifications same as above.
	 
	 
	 
	 

	 
	Back Cabinet: Providing and placing the modular back cabinet of approved make & model of required size. The top , side & front modesty specifications same as above.
	 
	 
	 
	 

	i
	SRM :  Equivalent to Godrej make 'premium suites' series 'Numero Uno' Model. consist of Main Desk+ ERU with ped + Mobile ped.  Main desk Size: 2290mm (W) x 1190mm (D) x 750mm (H), ERU size: 1380x480x700; mobile pedestal: 406x550x640
	1
	Nos
	
	

	ii
	DRM: Equivalent to Godrej make 'executive' series 'trident senior' Model. consist of main table with side credenza and pedestal & back storage. Table top Size: 1950mm (W) x 900mm (D) x 750mm (H). ERU size: 1050x450x705; mobile pedestal: 646H x 390W x 440D and HDU size: 1500 x 425 x 705.
	1
	Nos
	
	

	iii
	CM: Equivalent to Godrej make 'executive' series 'finesse' Model. consist of Main Desk + ERU with ped + Mobile pedestal + HDU.  Main desk Size: 1800 mm (W) x 900mm (D) x 740mm (H), ERU size: 1050x450x705; mobile pedestal: 646H x 390W x 440D and HDU size: 1280 x 425 x 705.
	4
	Nos
	
	

	 
	 
	 
	 
	 
	 

	j
	SWO / OFFICER COUNTERS
	 
	 
	 
	 

	 
	 Providing & fixing Officer tables as per design, of 2’-6” ht, 4'-6'' to 5'-0'' length and 2’-6’’' width. Two of the corners/edges will be curvilinear/straight in shape. The counters shall have the provision to adjust the key board on telescopic channels, drawer units,  trolley for CPU at bottom, cable manager and foot rest (3'x1.5'). The officer tables top shall be made of 25 mm thick BWR/BWP ply wood, with teak wood Gola of size 1½ ”x ¾ ”, which is to be polished as per color scheme. The sides and front modesty shall be made up of 19 mm thk. BWR/BWP plywood. The counter shall be finished with 1mm thick laminate of approved shade / colour, complete with all necessary hardware such as S.S.handles, magnet catchers, brass hinges, locks, etc. as per Bank’s approved brand/make. Inner surfaces of the table, counters etc. to have 0.8 mm laminated finish. The top shall have 8 mm thick float glass as per table top shape with hole for cable manager with pencil polish edges. 

	 
	 
	 
	 

	 
	Pedestal/Drawer Unit: The modular pedestal/drawer unit shall have outer dimensions of 680mm height x 360mm width x 450mm depth. The drawer unit shall consist of One pencil tray, 2 drawers and one filing box. It shall be provided with 2 lockable and two free twin wheeled castors. The pedestals shall have central locking mechanism. The drawers and filing box shall be mounted on telescopic ball bearing slides. 
	 
	 
	 
	 

	 
	CPU trolley: The CPU trolley shall be made of 0.8mm CRCA steel and should be adjustable to accommodate CPUs of various sizes. The CPU trolleys shall be provided with two lockable and two free twin wheeled castors. The CPU trolleys shall also be provided PVC foam gaskets of 4mm thickness to prevent any scratches on the CPU.
	 
	 
	 
	 

	 
	Table top size: 1500mm (L) x 750mm (W)
	12
	nos
	
	

	 
	Table top size: 1350mm (L) x 750mm (W)
	10
	nos
	
	

	 
	 
	 
	 
	
	

	k
	LINEAR COUNTERS WITH GLASS PARTITIONS- For R.C.C.
	 
	 
	 
	 

	 
	Providing & fixing Banking / Officer counters as per design, of 2’-6” ht and of 2'-0'' width. The counters shall have the provision to adjust the key board, drawers, storage complete shelf for CPU at bottom, cable manager and foot rest (3’X1.5’). The counters shall be made of 19mm thick BWR/BWP plywood, with teak wood Gola of size 1½ ”x ¾ ”, which is to be polished as per color scheme. The counter shall be finished with 1mm thick laminate of approved shade / colour, complete with all necessary hardware such as S.S.handles, magnet catchers, brass hinges, locks, etc. as per Bank’s approved brand/make. Inner surfaces of the table, counters etc. to have 0.8 mm laminated finish. Providing & fixing 12 mm glass partitions of approved make with pencil polish edges of curvilinear shape with SS fittings complete.
	28
	RFT
	
	

	 
	 
	 
	 
	 
	 

	l
	DAFTARI DESK WITH PIGEON HOLE
	 
	 
	 
	 

	 
	Providing & Fixing at site Daftari Table of size 7'-6'' x 2'-0'' working plane with 120 compartments Pigeon Hole made of 19 mm thick BWR grade Block Boards with approved color laminates inside/outside .Storage below as per the design & instruction of the Consultant.
	1
	Nos
	
	

	 
	 
	 
	 
	 
	 

	m
	CONFERENCE ROOM TABLE: Providing and placing of modular conference table of approved make & model height 750mm having top thickness 37.5 (18mm thk MDF + 18mm thk MDF+0.8mm decorative laminate+0.4mm Membrane Edge profile waterfall edge. 10mm radius on top edge and 5 mm at bottom. Understructure Legs Modesty Panel made from metal perforated having a straight profile with round edges. Nickel chrome plated slim legs.  Have access flaps mounted on table top with handy plug points. Complete in all respect in following sizes:
	 
	 
	 
	 

	
	Semi Modules (2 Seater) Radius 750mm, 1350mm (W): Equivalent model: Godrej make 'CONFERENCE TABLE' series 'talk modular-laminate' model. 
	2
	Nos
	
	

	
	Quad modules rectangular (2 seater) of size 1350mm (W) x 600mm (D): Equivalent model: Godrej make 'CONFERENCE TABLE' series 'talk modular-laminate' model. 
	8
	Nos
	
	

	 
	 
	 
	 
	 
	 

	n
	Showcase Unit: Providing & fixing in position SHOW CASE UNIT 1'9" deep made out of made of 19mm Boiling water resistant board (BWR grade IS 1659) for bottom, top, sides, & back with teak wood beading for all exposed surfaces. The shutters shall be made of 25 mm thick BWP boards as per the design & pattern & shall be fixed over 1”x1” teak wood frame section all around & shall be flush with the top edge. Showcase unit shall have 12 mm thick Glass shelves & Shutter. Fascia & top shall have 1.0 mm thick approved laminate finish. All inside surfaces are approved color Laminate. The length of cabinets may vary as per site conditions. Shutters shall have EBCO fittings, Godrej make locks & magnetic catcher, complete as per design & Consultant’s instruction. 
All hardware's as per approved make and specifications all edges of glass to be computer polished smooth. The rate shall include polishing of glass/mirror, cutting of holes for fittings, lights, etc., all hardware, adhesive, screws, accessories, lead and lift, finishes of hardware fittings to be considered from the material specifications as attached in the drawings, the details shown in the drawings, all as directed by EIC.
	 
	 
	 
	 

	
	Size: 2750mm(W)x525mm(D)x2400mm (H)
	1
	no
	
	

	 
	 
	 
	 
	Total=
	 

	
	
	
	
	
	

	
	Summary Sheet(PART-I) - Interior
	
	

	S.No.
	Items
	Amount (Rs.)
	
	

	1
	CIVIL /FAÇADE  WORKS
	
	
	

	2
	FALSE CEILING WORK
	
	
	

	3
	PAINTING WORKS
	
	
	

	4
	INTERIOR FURNISHING WORKS
	
	
	

	5
	 FURNITURE ITEMS
	
	
	

	
	Total=
	 
	
	


	BOQ SPECIFICATIONS OF ELECTRIFICATION, TELEPHONE, DATA, AIR CONDITIONING AND SECURITY SYSTEMS WORKS 

	S.NO
	 
	ITEM AND SPECIFICATION
	QTY
	UNIT
	RATE
	AMOUNT

	 
	 
	(A)ELECTRICAL WORKS
	 
	 
	 
	 

	 
	 
	ELECTRICAL 
	 
	 
	 
	 

	 
	 
	SUBHEAD  I (POINT WIRING)
	 
	 
	 
	 

	 
	 
	The rates for the point wiring shall include providing and fixing of following:
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 

	a.
	 
	Wiring of the point of any length from distribution board to point outlet including circuit wiring (i.e from DB to Switchboard)
	 
	 
	 
	 

	b.
	 
	Earthing of all switch box and all outlet boxes fitting, fans, 3rd pin of plug with 1.50mm copper wire.
	 
	 
	 
	 

	c.
	 
	Modular Switch/ Sockets of Standard make with necessary modular series cover plate and MS Boxes
	 
	 
	 
	 

	d.
	 
	Embedding all conduits in walls laying in slabs, above false ceiling or in floors including all accessories as required, cutting and refilling the chases with cement mortar.
	 
	 
	 
	 

	e
	 
	Providing, fixing Modular switches, sockets, M.S. boxes (1.6mm thick) draw boxes, G.I. Pull wires (where required), brass screws, ceiling rose/connector etc.
	 
	 
	 
	 

	f
	 
	Adopting separate and independent system of wiring for lighting, power (normal and essential supply). Wiring for following points using PVC insulted copper conductor wires of 650V/1100V grade in MMS grade-PVC conduit concealed/ exposed including switches & sockets as above.
	 
	 
	 
	 

	 
	 
	 LIGHT :(Maximum three points to be looped from primary)
	 
	 
	 
	 

	
	
	 POWER :( Maximum TWO points in one circuit)
	
	
	
	

	 INTERNAL WIRING
	 
	 
	 
	 

	1
	 
	POINT WIRING :
	 
	 
	 
	 

	 
	 
	Providing wiring ( supply, fixing, testing and comm. etc) for light point / Exhaust fan point / Call bell point/6A Switch-socket point etc with 2x1.5+1X1.5 sq mm FRLS PVC insulated copper conductor single core multi stranded wire in MMS grade-PVC conduit with conduit accessories like bend , junction box etc in concealed/surface manner as per site requirement with suitable Modular Switches with plate and metal / PVC box, ceiling rose , bulb holder etc including 1.5 sqmm PVC insulated copper earth wire etc complete as required. Wire colors : Red, Black, Green .Supplying, providing wiring (supply, fixing, testing and comm. etc) for  circuit with 2 x 2.5 + 1 x 2.5 sq mm  FRLS PVC insulated copper conductor single core multi stranded wire in MMS grade-PVC conduit   with conduit accessories like bend, junction box etc on surface / recessed manner etc ( Wiring from D.B. / Source to   Board/destination ) and making good all the damages, painting, cleaning the site etc complete as required as per site requirement and as directed 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 

	 
	a.
	Providing and fixing Primary light point
	40
	Nos.
	
	

	 
	b.
	Providing and fixing Secondary light point(Maximum three points to be looped from primary)
	80
	Nos.
	
	

	 
	c. 
	Plug point /ceiling Rose Point ( for wall fans/Exhaust fan)
	35
	Nos.
	
	

	
	
	Supply, fixing and commissioning of 1 No 6A multi Socket with 1 No. 6A switch (Modular type) with cover plate, sheet steel box / PVC modular box etc on surface / concealed manner I/c electrical connections and making good all the damages, painting, cleaning the site etc. complete as required as per site requirement and as directed.
	
	
	
	

	 
	d
	P&F bell point i/c of buzzer
	2
	Nos.
	
	

	 
	e
	6 AMP. POINTS ON SAME BOARD(Half point) :
	 
	 
	 
	 

	[image: image1.jpg]



 


	 
	Supply, fixing, testing and commissioning of 1 No 6 A Multi Socket with 1No. 6 A switch ( Modular type ) with cover plate , sheet steel box / PVC modular box etc. on surface / concealed manner I/c electrical connections and making good all the damages, painting, cleaning the site etc. complete as required as per site requirement and as directed.
	20
	Nos.
	
	

	 
	 f
	 Ceiling fan point (rate should include electronic fan speed regulator)
	5
	Nos. 
	
	

	2
	 
	16 AMP. POWER POINTS:(including circuit wiring)
	 
	 
	
	

	[image: image9.png]



 


	 
	Supply, fixing, testing and commissioning of 1 No 16 A switch & 1 No. six pin 6/16 Amp. Multi Socket   ( Modular Type ) with cover plate , sheet steel box etc on surface / concealed manner I/c electrical wiring with 2 x4 sqmm + 1 x 4 sqmm FRLS PVC insulated copper conductor single core multi stranded wire in MMS grade-PVC conduit with conduit accessories like bend, junction box etc on surface / recessed manner etc ( Wiring from D.B. / Source to Board to destination ) and making good all the damages, painting, cleaning the site etc complete as required as per site requirement and as directed.
	16
	Nos.
	
	

	3
	 
	AC POINTS :(including circuit wiring)
	 
	 
	 
	 

	 
	 
	Supply, Installation, Testing and commissioning of the surface / recess mounting distribution board with 20 A Metal plug and socket, with 25A/32A/40A SP MCB Incl. wiring with 2 X 4.0 sq mm + 1 X 4 sqmm PVC insulated copper conductor single core multi stranded wire in MMS grade-PVC conduit with conduit accessories like bend, junction box etc on surface / recessed manner etc ( Wiring from D.B. / Source to    Board/destination ) and making good all the damages, painting, cleaning the site etc complete as required as per site requirement and as directed.(MCB of C-Curve with S.C Capacity 10 kA)
	10
	Nos.
	
	

	 
	 
	 
	 
	 
	 
	 

	 PANELS AND D.B.'s
	 
	 
	 
	 

	4
	(A)
	MAIN PANEL/VTPN(4 WAY) :(With following minimum capacity)
	 
	 
	 
	 

	 
	 
	Supply, installation , testing and commissioning  of totally enclosed compartmentalized dust and vermin proof cubical segregated and modular in construction M.V. panel board wall mounted fabricated with14swg and 16swg of CRCA M.S. sheet duly painted with two coat of metal red oxide and two coat of fire resistance paint at inside and outside of the panel, bus-bar chamber ,outgoing switchgear etc. (all feeder unit Would be compartmentalized), color coded PVC sleeved vertical / horizontal bus bar of required size of length, ( bus-bar distances shall be minimum 32 mm ) insulators, hardware, neoprene gasket , hinged door, interconnecting single core multi strand lugged copper wire having current density of 2Amp/sqmm of suitable capacity & size with lugs from bus bar to switchgears / mccb / mcb or where ever required, two Earthing terminal busbar of size 25 x 5 mm with nut & bolts at out side of the panel , rating and name plates for all incoming & outgoings , two eye two nos eye bolts, wire mesh jali for ventilation etc comprising with the followings.
	 
	 
	 
	 

	 
	 
	NOTE:-
	 
	 
	 
	 

	 
	 
	Sheet 16 swg : panel sides, upper, lower and Ft. doors
	 
	 
	 
	 

	 
	 
	Sheet 16 swg : back side and compartments.
	 
	 
	 
	 

	 
	 
	Glande plates : 3 mm thick.
	 
	 
	 
	 

	 
	 
	Cable entry: Provision at bottom and  upper sides.
	 
	 
	 
	 

	 
	 
	Inside the panel: white colour paint.
	 
	 
	 
	 

	 
	 
	Outside the panel: Grey colour paint or as directed.
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 

	 
	 
	INCOMER 
	 
	 
	 
	 

	 
	 
	1 Nos 200 Amp MCCB, 25 KA- 4 Pole, C-curve
	 
	 
	 
	 

	 
	 
	1 Nos – 250 A TPN insulated Cupper Bus Bar 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 

	 
	 
	Set of Indicator Lamps
	 
	 
	 
	 

	 
	 
	Set of Voltmeter + Ammeter + Selector Switch
	 
	 
	 
	 

	 
	 
	OUTGOINGS
	 
	 
	 
	 

	 
	 
	4Nos- 63 Amp, TPMCB,C-curve
	 
	 
	 
	 

	 
	 
	SET AS ABOVE
	1
	Nos
	
	

	 
	 
	 
	 
	 
	 
	 

	 
	B
	SFU TPN 200 A with HRC fuses (just after meter and prior to Main Panel)
	1
	Nos
	
	

	 
	 
	 
	 
	 
	 
	 

	5
	 
	LIGHT DISTRIBUTION BOARD  
	 
	 
	 
	 

	 
	 
	Supply, Installation, Testing and commissioning of the  surface / recess mounting following way TPN MCB  three phase distribution board double door for single phase outgoing with IP 42 protection , direct on wall incl. the followings accessories 
	 
	 
	 
	 

	 
	 
	INCOMER
	 
	 
	 
	 

	 
	 
	1 No. TPN-RCBO/ELMCB 63 Amp ,100 ma sensitivity 
	 
	 
	 
	 

	 
	 
	OUTGOINGS
	 
	 
	 
	 

	 
	 
	18 Nos SPMCB 6/10/16 Amp, B-Curve
	 
	 
	 
	 

	 
	 
	SET AS ABOVE
	1
	Nos
	
	

	 
	 
	incl. Electrical connection ,Earthing, making good all the damages, painting, cleaning the site, etc complete as per site requirement and as directed. 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 

	6
	 
	AC DISTRIBUTION BOARD 
	 
	 
	 
	 

	 
	 
	Supply, Installation, Testing and commissioning of the  surface / recess mounting following way MCB  three phase distribution board double door for single phase outgoing with IP 42 protection , direct on wall incl. the followings accessories 
	 
	 
	 
	 

	 
	 
	INCOMER
	 
	 
	 
	 

	 
	 
	1 No. TPMCB 63Amp ,C-curve
	 
	 
	 
	 

	 
	 
	OUTGOINGS
	 
	 
	 
	 

	 
	 
	24 Nos SPMCB 25/32/40 Amp,C-curve
	 
	 
	 
	 

	 
	 
	SET AS ABOVE
	1
	Nos
	
	

	 
	 
	incl. Electrical connection ,earthing, making good all the damages, painting, cleaning the site, etc complete as per site requirement and as directed. 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 

	 
	 
	SUBHEAD IV : UPS WIRING
	 
	 
	 
	 

	7
	 
	U.P.S. DISTRIBUTION BOARD
	 
	 
	 
	 

	 
	 
	Supply, Installation, Testing and commissioning of the  surface / recess mounting following way Double door MCB D.B.- Single  phase distribution board ( Consumer unit )  for single phase out going with IP 42 protection incl. the  followings accessories – incl. Electrical connection ,earthing, making good all the damages, painting, cleaning the site, etc complete as per site requirement and as directed. 
	 
	 
	 
	 

	 
	a.
	INCOMER
	 
	 
	 
	 

	 
	 
	1 NOS63 A DP MCB
	 
	 
	 
	 

	 
	 
	OUTCOMER
	 
	 
	 
	 

	 
	 
	1 Nos- 63Amp DP MCB, 20 NOS 6/10/16 AMP SPMCB
	 
	 
	 
	 

	 
	 
	SET AS ABOVE
	1
	Nos
	
	

	 
	 
	 
	 
	 
	 
	 

	8
	 
	SPECIAL POINTS: ( UPS) any length(TO WORKSTATIONS)
	 
	 
	 
	 

	 
	 
	Supply, fixing, testing and commissioning of following Modular type switch socket with cover plate , sheet steel box etc on surface / concealed manner I/c electrical wiring with  2 X 2.5 sq mm + 1 X 2.5 sq mm FRLS  PVC insulated copper conductor single core multi stranded wire in rigid MMS grade PVC conduit with conduit accessories like bend, junction box etc on surface / recessed manner etc ( Wiring from D.B. / Source to    Board/destination ) and making good all the damages, painting, cleaning the site etc complete as required as per site requirement and as directed.
	 
	 
	 
	 

	 
	 
	1 Nos. 16 A Switch + 3 Nos. 6/16 A, 5 pin Socket.
	36
	Nos.
	
	

	 
	 
	 
	 
	 
	 
	 

	9
	 
	EARTHING 
	 
	 
	 
	 

	 
	 
	Preparation of the Earth station : ( as per I.S. 3043 )
	 
	 
	 
	 

	 
	 
	a). Excavation of rocky earth, soft murrum, hard  murrum etc. and back filling with black cotton soil for the earth station, the earth pit size is 1000 mm X 1000 mm X 2500 mm deep. 
	 
	 
	 
	 

	 
	 
	b). S/F of  Copper plate of size 600 X 600 X 3.00 mm
	 
	 
	 
	 

	 
	 
	c). Supply & fixing  25 mm X 5 mm , 3 mtrs copper strip
	 
	 
	 
	 

	 
	 
	from copper plate to earth terminal including
	 
	 
	 
	 

	 
	 
	brazing/welding at plate etc. 
	 
	 
	 
	 

	 
	 
	d). Supplying and laying in position 15 mm,2 mtrs  G.I. B class perforated pipe for watering.
	 
	 
	 
	 

	 
	 
	e). S/F of one set of reducer / funnel with mesh .
	 
	 
	 
	 

	 
	 
	f). S/F of the following in the earth station.
	 
	 
	 
	 

	 
	 
	i). 75 Kg. Charcoal.
	 
	 
	 
	 

	 
	 
	ii). 50 Kg. Original Salt.
	 
	 
	 
	 

	 
	 
	g). Construction of earth pit chamber incl. necessary brick work, concrete , plastering, S/F of C.I. cover of  size 12” X 12” complete as per site requirement with watering arrangement etc. complete..  
	2
	Nos.
	
	

	 
	 
	 
	 
	 
	 
	 

	10
	 
	Supplying and laying 25 X 3 mm copper strip direct on wall/ in ground with screws and washer including soldering / welding etc. if required..
	12
	M
	
	

	 
	 
	 
	 
	 
	 
	 

	11
	 
	Supply and laying of 6.0 sqmm PVC insulated copper wire from earth station to main panel board in 20 mm  GI Pipe including all materials, accessories etc. complete.
	90
	Mtrs.
	
	

	 
	 
	 
	 
	 
	 
	 

	 CABLING :
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 

	12
	 
	L.T.CABLES :
	 
	 
	 
	 

	 
	 
	Supply, laying, testing and commissioning of the following 1100 volt grade pvc insulated Al / Cu. Conductor armored cable inner and outer sheathed , along with the two run of G.I. earth wire i/c termination with brass gland and Al. lugs etc. complete as required.
	 
	 
	 
	 

	 
	 
	 On surface  :
	 
	 
	 
	 

	 
	 
	S/Fixing the cable on wall / column / beam / ceiling  / above false ceiling / existing trench etc incl. s/f of of saddles / spacers ( wherever required as per site conditions) and two run of G.I. earth wire along with the cable. Making good all the damages
	 
	 
	 
	 

	 
	a
	4 C x 16.0 sqmm armored copper cable  with 10 SWG 2 Nos G.I. wire for Electric room /Ups room
	30
	Mtrs.
	
	

	 
	 
	 
	 
	 
	
	

	 
	b
	 3.5 C X 50sqmm. Al. Armored .( with 10 SWG  2 Nos. G.I. wire ) from ELECTRIC METER to MAIN PANEL
	30
	Mtrs.
	
	

	 
	 
	 
	 
	 
	 
	 

	 TELEPHONE WIRING / CABLING SYSTEM.
	 
	 
	 
	 

	 
	 
	TELEPHONE POINT :
	 
	 
	 
	 

	13
	 
	Supplying, Installation, testing and commissioning of the telephone point with the followings -
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 

	 
	a.
	Two pair, 0.61 mm dia. telephone cable tinned copper conductor, P.V.C. insulated and sheathed , fire retarding, anti-termite, color coded twisted pairs and rip cord. 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 

	 
	b
	HMS Pvc pipe on beam /column / wall / floor etc. with all necessary materials i/c connections, identification by numbering etc. complete as required as per I.T.D. specification.
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 

	 
	c.
	Double outlet with shutter modular type Telephone Outlets ( RJ – 11 ) with suitable size PVC modular boxes complete as required .
	8
	Nos.
	
	

	 
	 
	 
	 
	 
	
	

	 
	d
	Single outlet with shutter modular type Telephone Outlets ( RJ – 11 ) with suitable size  PVC modular boxes complete as required .
	24
	Nos.
	
	

	14
	a
	Providing and fixing 50pair KRONE make telephone tag block with 20 pair module with termination and crimping complete and making good the surface as required/ directed.
	1
	Nos.
	
	

	 
	 
	 
	 
	 
	
	

	 
	b
	SITC of EPABX SYSTEM: 8 x 24 system with wiring, connections, installation complete with labeling also. Make: Matrix, Siemens or equivalent.
	1
	Nos.
	
	

	 
	 
	 
	 
	 
	 
	 

	 
	c
	Providing and fixing  10 pair armored tinned copper telephone cable in 32 mm PVC conduit from telephone utility junction box
	40
	Mtr
	
	

	TOTAL FOR ELECTRICAL WORKS (A) RS.
	     

	 
	 
	 
	 
	 
	 
	 

	(B)DATA CABELING WORKS

	 
	 
	COMPUTER CABLING SYSTEM.
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 

	 
	 
	COMPUTER POINT : I / O's :
	 
	 
	 
	 

	1
	a
	Supplying, Installation, testing and commissioning of the Computer point with the followings -
	 
	 
	 
	 

	[image: image10.png]



 


	 
	Four pair UTP CAT 6 LAN cable tinned copper conductor, P.V.C. insulated and sheathed, fire retarding, anti-termite, color coded twisted pairs and rip cord. (from server room switch to I/O outlet ) 
	 
	 
	 
	 

	 
	 
	HMS Pvc Pipe on beam /column / wall /  floor etc with all necessary materials i/c connections, identification by numbering etc complete as required as per At & T specification.
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	Single outlet with shutter modular type I / O's Outlets ( RJ – 45 ) with suitable size  PVC modular boxes complete as required
	40
	Nos.
	
	

	 
	 
	 
	 
	 
	
	

	 
	b
	Supply and Installation of following factory fabricated patch cords (UTP-CAT 6) complete with connectors and boots on both sides.
	 
	 
	
	

	 
	 
	Two Meter length
	32
	Nos.
	
	

	 
	 
	 
	 
	 
	
	

	 
	c
	20 years certification from DLINK of all Data nodes – PENTA Scanning with reports (to include ferruling and labeling)
	40
	Nos
	
	

	 
	 
	 
	 
	 
	 
	 

	TOTAL FOR COMPUTER NETWORKING (B) RS.
	

	 
	 
	 
	 
	 
	 
	 

	 SPECIFICATIONS FOR ELCETRICAL FITTINGS

	(C)ELECTRICAL FITTINGS/FIXTURES
	 
	 
	 
	 

	1
	 
	Supply, fixing, testing and commissioning of Recess/Surface mounted decorative luminaire with LED FIXTURES  with class I electrical safety, complete as required Fitting Dimensions : 
	 
	 
	 
	 

	 
	a
	  36-40 watts, Minimum 3500 lumens LED  size 600 X 600 X 80 mm (Approx.) : CRI>80, PF>0.9 Equivalent Model: Philips 35 S RC 380B (LED 'FULLGLOW' high efficiency series)
	50
	Nos.
	
	

	 
	 
	 
	 
	 
	
	

	 
	b
	12-13 w ,Minimum 1000 lumens LED ROUND DOWN LIGHTER Diameter  110-165mm,CRI>80,PF>0.9 Equivalent Model: Philips 9S DN 152B (GREEN LED Ultima  series)
	50
	Nos.
	
	

	 
	 
	 
	 
	 
	
	

	 
	c
	9-10 w  led  batten Light of  4'-0'' LENGTH
	20
	Nos.
	
	

	 
	 
	 
	 
	 
	 
	 

	 
	d
	LED rope lights with drivers of colour as approved by bank
	200
	mtrs
	
	

	 
	 
	 
	 
	 
	 
	 

	 
	e
	LED decorative luminaries various shapes as approved by bank. (Base rate: Rs. 1500.00)
	10
	nos
	
	

	 
	 
	 
	 
	 
	
	

	2
	a
	WALL BRACKET FAN
	 
	 
	
	

	 
	 
	Supply and fixing of the following fans Wall bracket fan white (400mm blade size)
	30
	Nos.
	
	

	
	
	
	
	
	
	

	 
	b
	CEILING FAN
	 
	 
	
	

	 
	 
	Supply and fixing of CEILING FAN 1200 MM Sweep five star rated.
	4
	Nos.
	
	

	
	
	
	
	
	
	

	 
	c
	EXHAUST FAN:
	 
	 
	
	

	 
	 
	Supply and fixing of the following single phase Exhaust Fan continuously rated, capacitor start and run type, totally enclosed and ruggedly built, pre lubricated double ball bearing, copper wounded, A & E class insulation, dynamically balanced, below 40 db sound level etc. Supplying & fixing of 300 dia Exhaust fans
	4
	Nos.
	
	

	TOTAL FOR ELECTRICAL FIXTURES(C) RS.
	

	

	(D)SPECIFICATIONS FOR AIR CONDITIONING WORK

	1
	 
	Supplying, Installation , testing & Commissioning of Air cooled type Indoor evaporating unit comprising of cooling coils, insulated sandwiched drain tray, 20 micron HDPE washable filters, blower, electrical junction box etc. Outdoor condensing unit comprising of Twin Rotary/Rotary compressors, condenser coils, propellor/axial fans etc. Necessary Refrigerant gas and oil Charge.
	 
	 
	 
	 

	 
	a
	7.5 TR HAT type air conditioner
	3
	Nos.
	
	

	 
	b
	5 TR HAT type air conditioner
	1
	Nos.
	
	

	 
	c
	3 TR Cassette type AC unit
	1
	Nos.
	
	

	 
	d
	1.5 TR Split type unit-3 star rated
	2
	Nos.
	
	

	 
	e
	1.0 TR Split type unit- 3 star rated
	2
	Nos.
	
	

	 
	e
	Stabilizers "V-Guard" make suitable for 1.5 tr /2 tr load
	4
	Nos.
	
	

	2
	 
	Low side Work
	 
	 
	
	

	 
	a
	Supply & fixing of Al. powder coated grill
	75
	Sqft.
	
	

	 
	b
	Supplying & Laying extra suitable Copper refrigerant piping with all required material.
	 
	 
	
	

	 
	i
	For HAT type air conditioner
	140
	Mtrs
	
	

	 
	ii
	For cassette AC 
	15
	Mtrs
	
	

	 
	iii
	For Split AC
	50
	Mtrs
	
	

	 
	c
	Supplying & Laying extra suitable PVC Drain piping with all required material.
	90
	Mtrs
	
	

	 
	d
	Supplying & Fixing suitable MS Stand with Cage with locking arrangement 
	 
	 
	
	

	 
	i
	For HAT type air conditioner
	3
	No.
	
	

	 
	ii
	For cassette AC 
	1
	No.
	
	

	 
	iii
	For Split AC
	4
	No.
	
	

	 
	e
	Supplying & Laying of power cable from indoor to outdoor 
	 
	 
	
	

	 
	i
	 For HAT type air conditioner
	150
	Mtrs
	
	

	 
	ii
	 For cassette AC 
	25
	Mtrs
	
	

	 
	iii
	For Split AC
	60
	Mtrs
	
	

	 
	f
	Canvas Connection from HAT indoor unit to grills
	12
	Nos.
	
	

	 
	g
	Core cutting in RCC for Copper piping/drain piping laying etc.
	15
	per Hole
	
	

	 
	h
	Mathadi Charges - Lifting, Shifting etc. of AC work
	1
	Lot
	
	

	 
	 
	TOTAL OF ' Air Conditioning' (D)Rs.
	 
	 
	 
	

	 
	 
	 
	 
	 
	 
	 

	E
	SITC of AUDIO/VIDEO SYSTEM

	 
	a
	Speakers- SITC of 4''/5'', 5-6 watts speaker with line matching transformer of Philips/Bosch make.
	10
	Nos
	
	

	 
	b
	Amplifier: SITC of 80 watts amplifier of "Philips/Bosch" make having facilitated with USB drive & FM.
	1
	Nos
	
	

	 
	c
	Wiring-2 Core 24/0.2 SWG flexible tinned copper polythene insulated & twin twisted copper cables for speakers volume control etc. through 20mm PVC conduits of medium gauge.
	175
	mtrs
	
	

	 
	d
	Projector Screen-manual: 8'x6' (approx.), wide format supported, pull down and self-lock type (Make: Draper/Dalite)
	2
	nos
	
	

	 
	e
	Supply & installation of custom Ceiling mounting kit (fixed type) for projector
	2
	nos
	
	

	 
	f
	3200 XGA projector Equivalent Model: Sony VPL-DX142- 2 Nos
	2
	nos
	
	

	 
	g
	Speakers- Wall/ceiling mount (Make: Studio Master Arc 60 series)
	8
	nos
	
	

	 
	h
	wireless microfone with Stand-Make: Studio Master Vak 10.c/10.d (with one chairman unit)
	10
	nos
	
	

	 
	i
	Wireless Hand held microfone Make: Studiomaster  Mic TR47H
	2
	nos
	
	

	 
	j
	Digital Audio mixer/Feedback reducer/RGB switcher/Amplifier. Make: Studio master
	1
	Nos
	
	

	 
	l
	AV Rack: For equipment storage
	1
	Nos
	
	

	 
	m
	Cable & connectors: HDMI, VGA and Audio cable, Power cable, Connectors
	 
	 
	
	

	 
	 
	(Note: Quantity to be supplied as per installation requirement for complete satisfactory installation. Total Lump sum rate to be quoted inclusive of all fittings)
	1
	LS
	
	

	 
	 
	TOTAL =
	 
	 
	
	

	 
	 
	 
	 
	 
	 
	 

	F
	FIRE ALARM & CCTV SYSTEM
	 
	 
	 
	 

	 
	a
	Fire Alarm system: Supplying, Installation, Testing & Commissioning of fire alarm panel having solid state ICS, Transistor LED, Smoke & Fire Control. Panel to be design & accept
signal from all types of automatic detector or manual actuators.
Panel shall be suitable for wall mounted & shall be provided with front glass lockable type. Each zone shall be isolated without effecting the other zone, automatic change over to secondary power source i.e. through sealed maintenance free battery in case of an interrupting in the incoming AC supply line. Test facility of each zone & BACKUP for 4 HOURS with rated sealed maintenance free dry type battery & battery charger shall be provided Hitachi make.
Fire Alarm Panel shall be of 4 zone.
voltmeter etc. (Make: - Zicom, System Sensor, Honeywell)
	1
	Nos
	
	

	 
	b
	Smoke detection system Supplying, Installation, Testing & Commissioning of smoke detection system below false ceiling & above where trap door is provided. Detector shall be dual chamber, dual source with LED provision. (Make: - Zicom, System Sensor, Honeywell)
	16
	Nos
	
	

	 
	c
	Heat Detector : As above in (b)
	2
	Nos
	
	

	 
	d
	Response Indicator: Supplying, Installation, Testing & Commissioning of response indicator to the above smoke detector having LED provision. (Make: - Zicom, System Sensor, Honeywell)
	2
	Nos
	
	

	 
	e
	Fire Pill Box: Supplying, Installation, Testing & Commissioning of fire pill box, break glass pipe, wall recess mounted in wall near exist. (Make: - Zicom, System Sensor, Honeywell)
	3
	Nos
	
	

	 
	f
	Hooter: S/I/T/Commissioning of Hooter of 90 db with Tone Generator. (Make: - Zicom, System Sensor, Honeywell)
	4
	Nos
	
	

	 
	g
	S/I/T/Commissioning of 1.1 Grade Copper conductors, PVC insulated cable of following size for fire alarm system. 2 Core X 1.5 Sq.mm. Copper YFY cable with termination (Make - Polycab / Finolex)
	90
	mtrs
	
	

	 
	h
	SITC of Dome Camera: 1/3” DIS, IR Vari focal lens, dome camera, 700 TVL, 2.8 mm to 12 mm 40m IR distance, IP66 ( Make: Thyonex, Hikvision, Samsung)
	12
	Nos
	
	

	 
	i
	SITC of IR Camera: 600 TVL, 1.3” DIS, 20m IR distance, ICR, 0.1 Lux/F1.2, 12VDC, wide operating temperature range (40 C to 60C), 2.8mm, 3.6mm, 6mm lens, Default 3.6mm / F1.8 lens)  ( Make: Thyonex, Hikvision, Samsung)
	4
	Nos
	
	

	 
	j
	SITC of 8 channel DVR: 8 Channel DVR D1 real time H.264, Front Panel 1UT, without Hard Disk, with networking facility  ( Make: Thyonex, Hikvision, Dahua)
	2
	Nos
	
	

	 
	k
	SITC of Power Supply : Power Supply for Camera 12v-1A - Pin Top type S
	4
	Nos
	
	

	 
	l
	SITC of Monitor: LED Monitor 21" with Wall Mount Facility ( Make: Samsung/Sony)
	1
	Nos
	
	

	 
	m
	SITC of Hard Disk-2 TB: (Make: Seagate/Samsung)
	2
	Nos
	
	

	 
	n
	SITC of Intrusion detection system: Control Panel with inbuilt buzzer, and Separate LCD Remote Key  Pad+ Motion Detector + Programmable arming/disarming , Wired Hooter with cabling
Smart Alert Facility
	1
	Nos
	
	

	 
	 
	TOTAL =
	 
	 
	 
	

	
	
	
	
	
	
	

	
	Summary Sheet (PART-II) - Electrical, Telephone, Data, A.C., & Security systems
	
	

	
	S.No.
	Items
	Amount (Rs.)
	
	

	
	1
	Total of Section A- Electrical DBs and points works
	
	
	

	
	2
	Total of Section B-Data Cabling
	
	
	

	
	3
	Total of Section C-Electrical Fixtures
	
	
	

	
	4
	Total of Section D-Air conditioning Works
	
	
	

	
	5
	Total of Section E-Audio/Video Items
	
	
	

	
	6
	Total of Section F-Security Items
	
	
	

	
	 
	Total(A+B+C+D+E+F)=
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